IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "0001"
Time stamp: "2020-02-17T13:50:35"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190327_2315(x64) - Exporter 20.0.0.377 - Alternate UI 20.0.0.377"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "User_05" of Organization (no name given)
  Owner history of Person "User_05" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1581943659 (2020-02-17T12:47:39Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "02 Level" | long name "02 Level" | object type "Level:8mm Head" | elevation 8000.
        contains 1 element
          1 x IFCSTAIR | object type "Cast-In-Place Stair:Monolithic Stair" | names: "Cast-In-Place Stair:Stair:389902" | parts: 2 IFCSTAIRFLIGHT, 1 IFCSLAB | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_StairCommon, Constraints, Dimensions, Identity Data
      IFCBUILDINGSTOREY "03 Level" | long name "03 Level" | object type "Level:8mm Head" | elevation 12000.
        contains 4 elements
          1 x IFCSTAIR | object type "Cast-In-Place Stair:Monolithic Stair" | names: "Cast-In-Place Stair:Stair:391172" | parts: 2 IFCSTAIRFLIGHT, 1 IFCSLAB | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_StairCommon, Constraints, Dimensions, Identity Data
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton 200mm" | object type "Floor:Vasbeton 200mm" | FLOOR | names: "Floor:Vasbeton 200mm:391211" | material: layers "Floor:Vasbeton 200mm" ("02_Vasbeton, helyszíni C40/50" 200.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton 150mm" | object type "Floor:Vasbeton 150mm" | FLOOR | names: "Floor:Vasbeton 150mm:391240" | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton 150mm" | object type "Floor:Vasbeton 150mm" | FLOOR | names: "Floor:Vasbeton 150mm:400813" | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, BaseQuantities
      IFCBUILDINGSTOREY "04 Roof" | long name "04 Roof" | object type "Level:8mm Head" | elevation 16000.
        contains 11 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton 200mm" | object type "Floor:Vasbeton 200mm" | FLOOR | names: "Floor:Vasbeton 200mm:392423" | material: layers "Floor:Vasbeton 200mm" ("02_Vasbeton, helyszíni C40/50" 200.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton 200mm" | object type "Floor:Vasbeton 200mm" | FLOOR | names: "Floor:Vasbeton 200mm:392434" | material: layers "Floor:Vasbeton 200mm" ("02_Vasbeton, helyszíni C40/50" 200.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton 200mm" | object type "Floor:Vasbeton 200mm" | FLOOR | names: "Floor:Vasbeton 200mm:400896" | material: layers "Floor:Vasbeton 200mm" ("02_Vasbeton, helyszíni C40/50" 200.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton 150mm" | object type "Floor:Vasbeton 150mm" | FLOOR | names: "Floor:Vasbeton 150mm:402501" | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton 150mm" | object type "Floor:Vasbeton 150mm" | FLOOR | names: "Floor:Vasbeton 150mm:402870" | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton 200mm" | object type "Floor:Vasbeton 200mm" | FLOOR | names: "Floor:Vasbeton 200mm:631273" | material: layers "Floor:Vasbeton 200mm" ("02_Vasbeton, helyszíni C40/50" 200.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton 150mm" | object type "Floor:Vasbeton 150mm" | FLOOR | names: "Floor:Vasbeton 150mm:643948" | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton 150mm" | object type "Floor:Vasbeton 150mm" | FLOOR | names: "Floor:Vasbeton 150mm:644097" | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton 150mm" | object type "Floor:Vasbeton 150mm" | FLOOR | names: "Floor:Vasbeton 150mm:644131" | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton 150mm" | object type "Floor:Vasbeton 150mm" | FLOOR | names: "Floor:Vasbeton 150mm:644161" | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton 150mm" | object type "Floor:Vasbeton 150mm" | FLOOR | names: "Floor:Vasbeton 150mm:644197" | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, BaseQuantities

Types
  IFCSLABTYPE "Floor:Vasbeton 200mm" | FLOOR | 1 occurrence | material: layers "Floor:Vasbeton 200mm" ("02_Vasbeton, helyszíni C40/50" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCSLABTYPE "Floor:Vasbeton 150mm" | FLOOR | 1 occurrence | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCSLABTYPE "Floor:Vasbeton 150mm" | FLOOR | 1 occurrence | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCSLABTYPE "Floor:Vasbeton 200mm" | FLOOR | 1 occurrence | material: layers "Floor:Vasbeton 200mm" ("02_Vasbeton, helyszíni C40/50" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCSLABTYPE "Floor:Vasbeton 200mm" | FLOOR | 1 occurrence | material: layers "Floor:Vasbeton 200mm" ("02_Vasbeton, helyszíni C40/50" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCSLABTYPE "Floor:Vasbeton 200mm" | FLOOR | 1 occurrence | material: layers "Floor:Vasbeton 200mm" ("02_Vasbeton, helyszíni C40/50" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCSLABTYPE "Floor:Vasbeton 150mm" | FLOOR | 1 occurrence | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCSLABTYPE "Floor:Vasbeton 150mm" | FLOOR | 1 occurrence | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCSLABTYPE "Floor:Vasbeton 200mm" | FLOOR | 1 occurrence | material: layers "Floor:Vasbeton 200mm" ("02_Vasbeton, helyszíni C40/50" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCSLABTYPE "Floor:Vasbeton 150mm" | FLOOR | 1 occurrence | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCSLABTYPE "Floor:Vasbeton 150mm" | FLOOR | 1 occurrence | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCSLABTYPE "Floor:Vasbeton 150mm" | FLOOR | 1 occurrence | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCSLABTYPE "Floor:Vasbeton 150mm" | FLOOR | 1 occurrence | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCSLABTYPE "Floor:Vasbeton 150mm" | FLOOR | 1 occurrence | material: layers "Floor:Vasbeton 150mm" ("02_Vasbeton, helyszíni C40/50" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other

Property sets
  Other(Type) | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    Category = "Runs" (IFCLABEL)
    Family Name = "Monolithic Run" (IFCTEXT)
  Other(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other(Type) | properties | on 2 objects (2 IFCSTAIR)
    Category = "Stairs" (IFCLABEL)
    Family Name = "Cast-In-Place Stair" (IFCTEXT)
  Other(Type) | properties | on 2 objects (2 IFCSLAB)
    Category = "Landings" (IFCLABEL)
    Family Name = "Monolithic Landing" (IFCTEXT)
  Other | properties | on 9 objects (9 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family = "Floor: Vasbeton 150mm" (IFCLABEL)
    Family and Type = "Floor: Vasbeton 150mm" (IFCLABEL)
    Type = "Floor: Vasbeton 150mm" (IFCLABEL)
    Type Id = "Floor: Vasbeton 150mm" (IFCLABEL)
  Other | properties | on 5 objects (5 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family = "Floor: Vasbeton 200mm" (IFCLABEL)
    Family and Type = "Floor: Vasbeton 200mm" (IFCLABEL)
    Type = "Floor: Vasbeton 200mm" (IFCLABEL)
    Type Id = "Floor: Vasbeton 200mm" (IFCLABEL)
  Other | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    Category = "Runs" (IFCLABEL)
    Family = "Monolithic Run: 150mm Depth" (IFCLABEL)
    Family and Type = "Monolithic Run: 150mm Depth" (IFCLABEL)
    Type = "Monolithic Run: 150mm Depth" (IFCLABEL)
    Type Id = "Monolithic Run: 150mm Depth" (IFCLABEL)
  Other | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 2 objects (2 IFCSTAIR)
    Category = "Stairs" (IFCLABEL)
    Family = "Cast-In-Place Stair: Monolithic Stair" (IFCLABEL)
    Family and Type = "Cast-In-Place Stair: Monolithic Stair" (IFCLABEL)
    Type = "Cast-In-Place Stair: Monolithic Stair" (IFCLABEL)
    Type Id = "Cast-In-Place Stair: Monolithic Stair" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCSLAB)
    Category = "Landings" (IFCLABEL)
    Family = "Monolithic Landing: 300mm Thickness" (IFCLABEL)
    Family and Type = "Monolithic Landing: 300mm Thickness" (IFCLABEL)
    Type = "Monolithic Landing: 300mm Thickness" (IFCLABEL)
    Type Id = "Monolithic Landing: 300mm Thickness" (IFCLABEL)
  Other | properties | on 14 type objects
    Category = "Floors" (IFCLABEL)
    Family Name = "Floor" (IFCTEXT)
  Identity Data(Type) | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "150mm Depth" (IFCTEXT)
  Identity Data(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data(Type) | properties | on 2 objects (2 IFCSTAIR)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Monolithic Stair" (IFCTEXT)
  Identity Data(Type) | properties | on 2 objects (2 IFCSLAB)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "300mm Thickness" (IFCTEXT)
  Graphics(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Graphics(Type) | properties | on 2 objects (2 IFCSTAIR)
    Cut Mark Type = "Stair Cut Mark: Single Zigzag" (IFCLABEL)
  Identity Data | properties | on 16 objects (14 IFCSLAB, 2 IFCSTAIR)
    Comments = "Szerkezeti födém" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "02 Level" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "03 Level" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "04 Roof" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 9 type objects
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Vasbeton 150mm" (IFCTEXT)
  Identity Data | properties | on 5 type objects
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Vasbeton 200mm" (IFCTEXT)
  Constraints(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Pset_ProductRequirements | properties | on 15 objects (14 IFCSLAB, 1 IFCOPENINGELEMENT) | on 14 type objects
    Category = "Floors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    Category = "Runs" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (2 IFCSTAIR)
    Category = "Stairs" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (2 IFCSLAB)
    Category = "Landings" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "02 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "03 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "04 Roof" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 9 objects (9 IFCSLAB) | on 9 type objects
    Reference = "Vasbeton 150mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 6 objects (5 IFCSLAB, 1 IFCOPENINGELEMENT) | on 5 type objects
    Reference = "Vasbeton 200mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    Reference = "150mm Depth" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCSTAIR)
    Reference = "Monolithic Stair" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCSLAB)
    Reference = "300mm Thickness" (IFCIDENTIFIER)
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 23. (IFCCOUNTMEASURE)
    NumberOfTreads = 21. (IFCCOUNTMEASURE)
    Reference = "Monolithic Stair" (IFCIDENTIFIER)
    RiserHeight = 173.913043478261 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 280. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairFlightCommon | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 23. (IFCCOUNTMEASURE)
    NumberOfTreads = 21. (IFCCOUNTMEASURE)
    Reference = "150mm Depth" (IFCIDENTIFIER)
    RiserHeight = 173.913043478261 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 280. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 280. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WaistThickness = 1500. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 750. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ReinforcementBarPitchOfSlab | properties | on 9 objects (9 IFCSLAB) | on 9 type objects
    Reference = "Vasbeton 150mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 5 objects (5 IFCSLAB) | on 5 type objects
    Reference = "Vasbeton 200mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "300mm Thickness" (IFCLABEL)
  Pset_SlabCommon | properties | on 7 objects (7 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Vasbeton 150mm" (IFCIDENTIFIER)
    ThermalTransmittance = 6.97333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Vasbeton 200mm" (IFCIDENTIFIER)
    ThermalTransmittance = 5.23 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "300mm Thickness" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Vasbeton 150mm" (IFCIDENTIFIER)
    ThermalTransmittance = 6.97333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Vasbeton 200mm" (IFCIDENTIFIER)
    ThermalTransmittance = 5.23 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 9 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Vasbeton 150mm" (IFCIDENTIFIER)
    ThermalTransmittance = 6.97333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 5 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Vasbeton 200mm" (IFCIDENTIFIER)
    ThermalTransmittance = 5.23 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  BaseQuantities | quantities | on 3 objects (3 IFCSLAB)
    GrossArea = 0.900000000000001 [SQUARE_METRE]
    GrossVolume = 135.000000000001 [CUBIC_METRE]
    NetArea = 2.43 [SQUARE_METRE]
    NetVolume = 0.135000000000001 [CUBIC_METRE]
    Perimeter = 4200. [MILLI METRE]
    Width = 150.000000000001 [MILLI METRE]
  BaseQuantities | quantities | on 2 objects (2 IFCSLAB)
    NetArea = 366.6592 [SQUARE_METRE]
    NetVolume = 35.38272 [CUBIC_METRE]
    Perimeter = 64160.0000000001 [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    NetArea = 41.7882728147117 [SQUARE_METRE]
    NetVolume = 3.83292013026833 [CUBIC_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    NetArea = 41.7882728147118 [SQUARE_METRE]
    NetVolume = 3.83292013026834 [CUBIC_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    NetArea = 79.4279999999997 [SQUARE_METRE]
    NetVolume = 5.3235 [CUBIC_METRE]
    Perimeter = 56319.9999999999 [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    NetArea = 82.2439999999997 [SQUARE_METRE]
    NetVolume = 7.09799999999997 [CUBIC_METRE]
    Perimeter = 56319.9999999999 [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    NetArea = 101.01285834302 [SQUARE_METRE]
    NetVolume = 7.03033937572655 [CUBIC_METRE]
    Perimeter = 48499.9999999998 [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Area = 14.7872708284895 [SQUARE_METRE]
    Depth = 200. [MILLI METRE]
  BaseQuantities: 6 more contents on 6 objects not shown
  Constraints | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    Location Line = "Run: Left" (IFCIDENTIFIER)
    Relative Base Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Relative Top Height = 2086.95652173913 (IFCLENGTHMEASURE) [MILLI METRE]
    Run Height = 2086.95652173913 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    Location Line = "Run: Left" (IFCIDENTIFIER)
    Relative Base Height = 2086.95652173913 (IFCLENGTHMEASURE) [MILLI METRE]
    Relative Top Height = 4000. (IFCLENGTHMEASURE) [MILLI METRE]
    Run Height = 1913.04347826087 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 2 objects (2 IFCSLAB)
    Relative Height = 2086.95652173913 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 2 objects (2 IFCSLAB)
    Height Offset From Level = -190. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: 03 Level" (IFCLABEL)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints | properties | on 2 objects (2 IFCSLAB)
    Height Offset From Level = -140. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: 04 Roof" (IFCLABEL)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCSTAIR)
    Base Level = "Level: 02 Level" (IFCLABEL)
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Desired Stair Height = 4000. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = "Level: 03 Level" (IFCLABEL)
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCSTAIR)
    Base Level = "Level: 03 Level" (IFCLABEL)
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Desired Stair Height = 4000. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = "Level: 04 Roof" (IFCLABEL)
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCSLAB)
    Height Offset From Level = -140. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: 03 Level" (IFCLABEL)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints: 12 more contents on 12 objects not shown
  Dimensions | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (2 IFCSTAIR)
    Actual Number of Risers = 23 (IFCINTEGER)
    Actual Riser Height = 173.913043478261 (IFCLENGTHMEASURE) [MILLI METRE]
    Actual Tread Depth = 280. (IFCLENGTHMEASURE) [MILLI METRE]
    Desired Number of Risers = 23 (IFCINTEGER)
    Tread/Riser Start Number = 1 (IFCINTEGER)
  Dimensions | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    Actual Number of Risers = 12 (IFCINTEGER)
    Actual Number of Treads = 11 (IFCINTEGER)
    Actual Riser Height = 173.913043478261 (IFCLENGTHMEASURE) [MILLI METRE]
    Actual Run Width = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
    Actual Tread Depth = 280. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    Actual Number of Risers = 11 (IFCINTEGER)
    Actual Number of Treads = 10 (IFCINTEGER)
    Actual Riser Height = 173.913043478261 (IFCLENGTHMEASURE) [MILLI METRE]
    Actual Run Width = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
    Actual Tread Depth = 280. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (2 IFCSLAB)
    Total Thickness = 300. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCSLAB)
    Area = 176.9136 (IFCAREAMEASURE) [SQUARE_METRE]
    Elevation at Bottom = 11660. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top = 11860. (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter = 64160.0000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 35.38272 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCSLAB)
    Area = 35.4899999999998 (IFCAREAMEASURE) [SQUARE_METRE]
    Elevation at Bottom = 11660. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top = 11810. (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter = 56319.9999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 5.3235 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCSLAB)
    Area = 176.9136 (IFCAREAMEASURE) [SQUARE_METRE]
    Elevation at Bottom = 15660. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top = 15860. (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter = 64160.0000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 35.38272 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 11 more contents on 11 objects not shown
  Phasing | properties | on 22 objects (16 IFCSLAB, 4 IFCSTAIRFLIGHT, 2 IFCSTAIR)
    Phase Created = "Phase 1" (IFCLABEL)
  Structural | properties | on 14 objects (14 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Structural | properties | on 2 objects (2 IFCSTAIR)
    Rebar Cover = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
  Construction | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    Begin with Riser = TRUE (IFCBOOLEAN)
    End with Riser = TRUE (IFCBOOLEAN)
    Extend Below Riser Base = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    Begin with Riser = TRUE (IFCBOOLEAN)
    End with Riser = TRUE (IFCBOOLEAN)
  Construction | properties | on 9 type objects
    Default Thickness = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Interior" (IFCIDENTIFIER)
  Construction | properties | on 5 type objects
    Default Thickness = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Interior" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 15 objects (14 IFCSLAB, 1 IFCOPENINGELEMENT) | on 14 type objects
    Roughness = 914.4 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "Vasbeton 200mm" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "02 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "03 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "04 Roof" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 3 (IFCINTEGER)
  Calculation Rules(Type) | properties | on 2 objects (2 IFCSTAIR)
    Maximum Riser Height = 180. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Run Width = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Tread Depth = 280. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    Structural Depth = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Underside Surface = "Smooth" (IFCIDENTIFIER)
  Construction(Type) | properties | on 2 objects (2 IFCSTAIR)
    Function = "Interior" (IFCIDENTIFIER)
    Landing Type = "Monolithic Landing: 300mm Thickness" (IFCLABEL)
    Run Type = "Monolithic Run: 150mm Depth" (IFCLABEL)
  Construction(Type) | properties | on 2 objects (2 IFCSLAB)
    Monolithic Thickness = 300. (IFCLENGTHMEASURE) [MILLI METRE]
  Supports(Type) | properties | on 2 objects (2 IFCSTAIR)
    Left Lateral Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Support = "None" (IFCIDENTIFIER)
    Middle Support = FALSE (IFCBOOLEAN)
    Middle Support Number = 0 (IFCINTEGER)
    Right Lateral Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Support = "None" (IFCIDENTIFIER)
  Materials and Finishes(Type) | properties | on 6 objects (4 IFCSTAIRFLIGHT, 2 IFCSLAB)
    Monolithic Material = "Concrete, Cast In Situ" (IFCLABEL)
  Risers(Type) | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    Riser = FALSE (IFCBOOLEAN)
    Riser Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Riser To Tread Connection = "Extend Riser Behind Tread" (IFCIDENTIFIER)
    Slanted = FALSE (IFCBOOLEAN)
  Treads(Type) | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    Apply Nosing Profile = "Front Only" (IFCIDENTIFIER)
    Nosing Length = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tread = FALSE (IFCBOOLEAN)
    Tread Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Treads(Type) | properties | on 2 objects (2 IFCSLAB)
    Same as Run = TRUE (IFCBOOLEAN)
  Analytical Properties | properties | on 9 type objects
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 6.97333333333333 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 0.1434034416826 (IFCREAL)
    Thermal mass = 226665. (IFCREAL)
  Analytical Properties | properties | on 5 type objects
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 5.23 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 0.191204588910134 (IFCREAL)
    Thermal mass = 302220. (IFCREAL)
  Graphics | properties | on 14 type objects
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Materials and Finishes | properties | on 14 type objects
    Structural Material = "02_Vasbeton, helyszíni C40/50" (IFCLABEL)

Other addresses and roles
  2 x postal address: "Enter address here", "Boston", "MA"