IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "0001"
Time stamp: "2020-02-17T13:59:50"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190327_2315(x64) - Exporter 20.0.0.377 - Alternate UI 20.0.0.377"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "User_05" of Organization (no name given)
  Owner history of Person "User_05" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1581943659 (2020-02-17T12:47:39Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "02 Level" | long name "02 Level" | object type "Level:8mm Head" | elevation 8000.
        contains 13 elements
          6 x IFCWALL | type IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" | object type "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" | names: "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés:389882", "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés:389884", "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés:389886" (+3 more) | material: materials ("03_Vakolat", "04_Austrotherm AT-H80 homlokzati hőszigetelő lemez", "02_Porotherm 30 N+F tégla", "03_Vakolat"); layers "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" ("03_Vakolat" 10., "04_Austrotherm AT-H80 homlokzati hőszigetelő lemez" 120., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" | object type "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" | names: "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés:389885", "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés:389945" | material: layers "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" ("03_Vakolat" 10., "04_Austrotherm AT-H80 homlokzati hőszigetelő lemez" 120., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" | object type "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" | names: "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat:389900", "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat:389938" | material: materials ("03_Vakolat", "02_Porotherm 30 N+F tégla", "03_Vakolat"); layers "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" ("03_Vakolat" 10., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" | object type "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" | names: "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat:389901", "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat:389957" | material: layers "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" ("03_Vakolat" 10., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal+2x12 cm hőszigetelés" | object type "Basic Wall:00_Külső vázkerámia fal+2x12 cm hőszigetelés" | names: "Basic Wall:00_Külső vázkerámia fal+2x12 cm hőszigetelés:389942" | material: layers "Basic Wall:00_Külső vázkerámia fal+2x12 cm hőszigetelés" ("03_Vakolat" 10., "06_ APP Modifikált bitumenes lemez" 10., "04_Austrotherm AT-H80 homlokzati hőszigetelő lemez" 120., "02_Porotherm 30 N+F tégla" 300., "04_Austrotherm EPS AT-L2 lépéshangszigetelő lemez" 120., "03_Vakolat" 10.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
      IFCBUILDINGSTOREY "03 Level" | long name "03 Level" | object type "Level:8mm Head" | elevation 12000.
        contains 25 elements
          6 x IFCWALL | type IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" | object type "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" | names: "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés:391152", "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés:391153", "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés:391154" (+3 more) | material: layers "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" ("03_Vakolat" 10., "04_Austrotherm AT-H80 homlokzati hőszigetelő lemez" 120., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" | object type "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" | names: "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés:391155", "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés:391215" | material: layers "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" ("03_Vakolat" 10., "04_Austrotherm AT-H80 homlokzati hőszigetelő lemez" 120., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" | object type "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" | names: "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat:391170", "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat:391208" | material: layers "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" ("03_Vakolat" 10., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" | object type "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" | names: "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat:391171", "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat:391227" | material: layers "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" ("03_Vakolat" 10., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:00_Külső vasbeton fal+vakolat" | object type "Basic Wall:00_Külső vasbeton fal+vakolat" | names: "Basic Wall:00_Külső vasbeton fal+vakolat:391253", "Basic Wall:00_Külső vasbeton fal+vakolat:391254", "Basic Wall:00_Külső vasbeton fal+vakolat:391262" (+6 more) | material: layers "Basic Wall:00_Külső vasbeton fal+vakolat" ("03_Vakolat, barnára festve" 15., "02_Vasbeton, helyszíni C40/55" 50., "03_Vakolat, barnára festve" 15.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Függönyfal" | object type "Curtain Wall:Függönyfal" | names: "Curtain Wall:Függönyfal:391609", "Curtain Wall:Függönyfal:393201" | parts: 32 IFCMEMBER, 8 IFCPLATE, 2 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Horizontal Grid
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:00_Külső vasbeton fal+vakolat" | object type "Basic Wall:00_Külső vasbeton fal+vakolat" | names: "Basic Wall:00_Külső vasbeton fal+vakolat:400831" | material: layers "Basic Wall:00_Külső vasbeton fal+vakolat" ("03_Vakolat, barnára festve" 15., "02_Vasbeton, helyszíni C40/55" 50., "03_Vakolat, barnára festve" 15.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal+2x12 cm hőszigetelés" | object type "Basic Wall:00_Külső vázkerámia fal+2x12 cm hőszigetelés" | names: "Basic Wall:00_Külső vázkerámia fal+2x12 cm hőszigetelés:402918" | material: layers "Basic Wall:00_Külső vázkerámia fal+2x12 cm hőszigetelés" ("03_Vakolat" 10., "06_ APP Modifikált bitumenes lemez" 10., "04_Austrotherm AT-H80 homlokzati hőszigetelő lemez" 120., "02_Porotherm 30 N+F tégla" 300., "04_Austrotherm EPS AT-L2 lépéshangszigetelő lemez" 120., "03_Vakolat" 10.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
      IFCBUILDINGSTOREY "04 Roof" | long name "04 Roof" | object type "Level:8mm Head" | elevation 16000.
        contains 33 elements
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" | object type "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" | names: "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat:392557", "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat:392558", "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat:392559" (+1 more) | material: layers "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" ("03_Vakolat" 10., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" | object type "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" | names: "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés:392766" | material: layers "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" ("03_Vakolat" 10., "04_Austrotherm AT-H80 homlokzati hőszigetelő lemez" 120., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          13 x IFCWALL | type IFCWALLTYPE "Basic Wall:00_Külső beton fal+2x12 cm szigetelés" | object type "Basic Wall:00_Külső beton fal+2x12 cm szigetelés" | names: "Basic Wall:00_Külső beton fal+2x12 cm szigetelés:393874", "Basic Wall:00_Külső beton fal+2x12 cm szigetelés:393937", "Basic Wall:00_Külső beton fal+2x12 cm szigetelés:394048" (+10 more) | material: materials ("03_Vakolat", "06_ APP Modifikált bitumenes lemez", "04_Austrotherm AT-H80 homlokzati hőszigetelő lemez", "02_Vasbeton, helyszíni C40/55", "04_Austrotherm EPS AT-L2 lépéshangszigetelő lemez", "03_Vakolat"); layers "Basic Wall:00_Külső beton fal+2x12 cm szigetelés" ("03_Vakolat" 10., "06_ APP Modifikált bitumenes lemez" 10., "04_Austrotherm AT-H80 homlokzati hőszigetelő lemez" 120., "02_Vasbeton, helyszíni C40/55" 300., "04_Austrotherm EPS AT-L2 lépéshangszigetelő lemez" 120., "03_Vakolat" 10.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat+szigetelés" | object type "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat+szigetelés" | names: "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat+szigetelés:402417" | material: materials ("03_Vakolat", "06_ APP Modifikált bitumenes lemez", "02_Porotherm 30 N+F tégla", "03_Vakolat") | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat+szigetelés" | object type "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat+szigetelés" | names: "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat+szigetelés:402418", "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat+szigetelés:402419", "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat+szigetelés:402859" | material: layers "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat+szigetelés" ("03_Vakolat" 10., "06_ APP Modifikált bitumenes lemez" 10., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:00_Külső vakolat" | object type "Basic Wall:00_Külső vakolat" | names: "Basic Wall:00_Külső vakolat:403725", "Basic Wall:00_Külső vakolat:403808", "Basic Wall:00_Külső vakolat:404003" (+4 more) | material: layers "Basic Wall:00_Külső vakolat" ("03_Vakolat" 10.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:00_Külső beton fal+12 cm hőszigetelés 2" | object type "Basic Wall:00_Külső beton fal+12 cm hőszigetelés 2" | names: "Basic Wall:00_Külső beton fal+12 cm hőszigetelés 2:675779" | material: layers "Basic Wall:00_Külső beton fal+12 cm hőszigetelés 2" ("03_Vakolat" 10., "04_Austrotherm AT-H80 homlokzati hőszigetelő lemez" 120., "02_Vasbeton, helyszíni C40/55" 300., "03_Vakolat" 10.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:00_Külső beton fal 300 mm+vakolat" | object type "Basic Wall:00_Külső beton fal 300 mm+vakolat" | names: "Basic Wall:00_Külső beton fal 300 mm+vakolat:675924", "Basic Wall:00_Külső beton fal 300 mm+vakolat:675997", "Basic Wall:00_Külső beton fal 300 mm+vakolat:676050" | material: materials ("03_Vakolat", "02_Vasbeton, helyszíni C40/55", "03_Vakolat"); layers "Basic Wall:00_Külső beton fal 300 mm+vakolat" ("03_Vakolat" 10., "02_Vasbeton, helyszíni C40/55" 300., "03_Vakolat" 10.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural

Types
  IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" | STANDARD | 17 occurrences | material: layers "Basic Wall:00_Külső vázkerámia fal+12 cm hőszigetelés" ("03_Vakolat" 10., "04_Austrotherm AT-H80 homlokzati hőszigetelő lemez" 120., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" | STANDARD | 12 occurrences | material: layers "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat" ("03_Vakolat" 10., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal+2x12 cm hőszigetelés" | STANDARD | 2 occurrences | material: layers "Basic Wall:00_Külső vázkerámia fal+2x12 cm hőszigetelés" ("03_Vakolat" 10., "06_ APP Modifikált bitumenes lemez" 10., "04_Austrotherm AT-H80 homlokzati hőszigetelő lemez" 120., "02_Porotherm 30 N+F tégla" 300., "04_Austrotherm EPS AT-L2 lépéshangszigetelő lemez" 120., "03_Vakolat" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:00_Külső vasbeton fal+vakolat" | STANDARD | 10 occurrences | material: layers "Basic Wall:00_Külső vasbeton fal+vakolat" ("03_Vakolat, barnára festve" 15., "02_Vasbeton, helyszíni C40/55" 50., "03_Vakolat, barnára festve" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCCURTAINWALLTYPE "Curtain Wall:Függönyfal" | 2 occurrences | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid, Pset_CurtainWallCommon
  IFCWALLTYPE "Basic Wall:00_Külső beton fal+2x12 cm szigetelés" | STANDARD | 13 occurrences | material: layers "Basic Wall:00_Külső beton fal+2x12 cm szigetelés" ("03_Vakolat" 10., "06_ APP Modifikált bitumenes lemez" 10., "04_Austrotherm AT-H80 homlokzati hőszigetelő lemez" 120., "02_Vasbeton, helyszíni C40/55" 300., "04_Austrotherm EPS AT-L2 lépéshangszigetelő lemez" 120., "03_Vakolat" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat+szigetelés" | STANDARD | 4 occurrences | material: layers "Basic Wall:00_Külső vázkerámia fal 300 mm+vakolat+szigetelés" ("03_Vakolat" 10., "06_ APP Modifikált bitumenes lemez" 10., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:00_Külső vakolat" | STANDARD | 7 occurrences | material: layers "Basic Wall:00_Külső vakolat" ("03_Vakolat" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:00_Külső beton fal+12 cm hőszigetelés 2" | STANDARD | 1 occurrence | material: layers "Basic Wall:00_Külső beton fal+12 cm hőszigetelés 2" ("03_Vakolat" 10., "04_Austrotherm AT-H80 homlokzati hőszigetelő lemez" 120., "02_Vasbeton, helyszíni C40/55" 300., "03_Vakolat" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:00_Külső beton fal 300 mm+vakolat" | STANDARD | 3 occurrences | material: layers "Basic Wall:00_Külső beton fal 300 mm+vakolat" ("03_Vakolat" 10., "02_Vasbeton, helyszíni C40/55" 300., "03_Vakolat" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other

Property sets
  Other | properties | on 32 objects (32 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
    Family = "Rectangular Mullion: 50 x 150mm" (IFCLABEL)
    Family and Type = "Rectangular Mullion: 50 x 150mm" (IFCLABEL)
    Host Id = "Curtain Wall: Függönyfal" (IFCLABEL)
    Type = "Rectangular Mullion: 50 x 150mm" (IFCLABEL)
    Type Id = "Rectangular Mullion: 50 x 150mm" (IFCLABEL)
  Other | properties | on 17 objects (13 IFCWALL, 4 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: 00_Külső vázkerámia fal+12 cm hőszigetelés" (IFCLABEL)
    Family and Type = "Basic Wall: 00_Külső vázkerámia fal+12 cm hőszigetelés" (IFCLABEL)
    Type = "Basic Wall: 00_Külső vázkerámia fal+12 cm hőszigetelés" (IFCLABEL)
    Type Id = "Basic Wall: 00_Külső vázkerámia fal+12 cm hőszigetelés" (IFCLABEL)
  Other | properties | on 13 objects (13 IFCWALL)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: 00_Külső beton fal+2x12 cm szigetelés" (IFCLABEL)
    Family and Type = "Basic Wall: 00_Külső beton fal+2x12 cm szigetelés" (IFCLABEL)
    Type = "Basic Wall: 00_Külső beton fal+2x12 cm szigetelés" (IFCLABEL)
    Type Id = "Basic Wall: 00_Külső beton fal+2x12 cm szigetelés" (IFCLABEL)
  Other | properties | on 12 objects (8 IFCWALLSTANDARDCASE, 4 IFCWALL)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: 00_Külső vázkerámia fal 300 mm+vakolat" (IFCLABEL)
    Family and Type = "Basic Wall: 00_Külső vázkerámia fal 300 mm+vakolat" (IFCLABEL)
    Type = "Basic Wall: 00_Külső vázkerámia fal 300 mm+vakolat" (IFCLABEL)
    Type Id = "Basic Wall: 00_Külső vázkerámia fal 300 mm+vakolat" (IFCLABEL)
  Other | properties | on 10 objects (9 IFCWALLSTANDARDCASE, 1 IFCWALL)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: 00_Külső vasbeton fal+vakolat" (IFCLABEL)
    Family and Type = "Basic Wall: 00_Külső vasbeton fal+vakolat" (IFCLABEL)
    Type = "Basic Wall: 00_Külső vasbeton fal+vakolat" (IFCLABEL)
    Type Id = "Basic Wall: 00_Külső vasbeton fal+vakolat" (IFCLABEL)
  Other | properties | on 8 objects (8 IFCPLATE)
    Category = "Curtain Panels" (IFCLABEL)
    Family = "System Panel: Glazed" (IFCLABEL)
    Family and Type = "System Panel: Glazed" (IFCLABEL)
    Host Id = "Curtain Wall: Függönyfal" (IFCLABEL)
    Type = "System Panel: Glazed" (IFCLABEL)
    Type Id = "System Panel: Glazed" (IFCLABEL)
  Other | properties | on 7 objects (7 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: 00_Külső vakolat" (IFCLABEL)
    Family and Type = "Basic Wall: 00_Külső vakolat" (IFCLABEL)
    Type = "Basic Wall: 00_Külső vakolat" (IFCLABEL)
    Type Id = "Basic Wall: 00_Külső vakolat" (IFCLABEL)
  Other | properties | on 4 objects (3 IFCWALLSTANDARDCASE, 1 IFCWALL)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: 00_Külső vázkerámia fal 300 mm+vakolat+szigetelés" (IFCLABEL)
    Family and Type = "Basic Wall: 00_Külső vázkerámia fal 300 mm+vakolat+szigetelés" (IFCLABEL)
    Type = "Basic Wall: 00_Külső vázkerámia fal 300 mm+vakolat+szigetelés" (IFCLABEL)
    Type Id = "Basic Wall: 00_Külső vázkerámia fal 300 mm+vakolat+szigetelés" (IFCLABEL)
  Other: 10 more contents on 17 objects not shown
  BaseQuantities | quantities | on 32 objects (32 IFCMEMBER)
    CrossSectionArea = 15.36 [SQUARE_METRE]
    Length = 6400. [MILLI METRE]
  BaseQuantities | quantities | on 4 objects (4 IFCOPENINGELEMENT)
    Depth = 3048. [MILLI METRE]
    Height = 1200. [MILLI METRE]
    Width = 1500. [MILLI METRE]
  BaseQuantities | quantities | on 3 objects (3 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 1.02399999999998 [SQUARE_METRE]
    Height = 4000. [MILLI METRE]
    Length = 3199.99999999998 [MILLI METRE]
    NetSideArea = 12.7999999999999 [SQUARE_METRE]
    NetSideArea = 12799999.9999999 [SQUARE_METRE]
    NetVolume = 3.94719999999993 [CUBIC_METRE]
    NetVolume = 4095999999.99997 [CUBIC_METRE]
    Width = 320. [MILLI METRE]
  BaseQuantities | quantities | on 2 objects (2 IFCDOOR)
    Area = 15.36 [SQUARE_METRE]
  BaseQuantities | quantities | on 2 objects (2 IFCOPENINGELEMENT)
    Depth = 329.999999999994 [MILLI METRE]
    Height = 999.234003431778 [MILLI METRE]
    Width = 750.000000000001 [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Depth = 3048. [MILLI METRE]
    Height = 900.000000000003 [MILLI METRE]
    Width = 2142. [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 1.73360000000002 [SQUARE_METRE]
    Height = 4000. [MILLI METRE]
    Length = 3940.00000000002 [MILLI METRE]
    NetSideArea = 13.9600000000001 [SQUARE_METRE]
    NetSideArea = 15760000.0000001 [SQUARE_METRE]
    NetVolume = 6.14240000000009 [CUBIC_METRE]
    NetVolume = 6934400000.00003 [CUBIC_METRE]
    Width = 440. [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 0.84074999999998 [SQUARE_METRE]
    Height = 4000. [MILLI METRE]
    Length = 1474.99999999999 [MILLI METRE]
    NetSideArea = 5.52324999999994 [SQUARE_METRE]
    NetSideArea = 5899999.99999994 [SQUARE_METRE]
    NetVolume = 3.14825249999997 [CUBIC_METRE]
    NetVolume = 3362999999.99997 [CUBIC_METRE]
    Width = 570. [MILLI METRE]
  BaseQuantities: 29 more contents on 29 objects not shown
  Identity Data | properties | on 71 objects (35 IFCWALL, 34 IFCWALLSTANDARDCASE, 2 IFCCURTAINWALL)
    Comments = "Külső fal" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCDOOR)
    Comments = "Nyílászáró" (IFCTEXT)
    Mark = "98" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCDOOR)
    Comments = "Nyílászáró" (IFCTEXT)
    Mark = "131" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "02 Level" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "03 Level" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "04 Roof" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B2010154" (IFCTEXT)
    Assembly Description = "Ext. Wall - Brick Cavity" (IFCTEXT)
    Type Comments = "F-K2-04" (IFCTEXT)
    Type Name = "00_Külső vázkerámia fal+12 cm hőszigetelés" (IFCTEXT)
  Identity Data: 9 more contents on 0 objects not shown
  Constraints | properties | on 42 objects (32 IFCMEMBER, 8 IFCPLATE, 2 IFCDOOR)
    Level = "Level: 03 Level" (IFCLABEL)
  Constraints | properties | on 11 objects (7 IFCWALL, 4 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: 03 Level" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -340. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Interior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 04 Roof" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = -340. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 4000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 9 objects (9 IFCWALL)
    Base Constraint = "Level: 04 Roof" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -340. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Interior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 04 Roof" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 1540. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 8 objects (5 IFCWALL, 3 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: 02 Level" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -340. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Interior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 03 Level" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = -340. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 4000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 7 objects (7 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: 04 Roof" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -465. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Interior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 04 Roof" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = -340.000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 125. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 5 objects (3 IFCWALL, 2 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: 02 Level" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -339.999999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Interior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 03 Level" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = -340. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 4000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 5 objects (4 IFCWALLSTANDARDCASE, 1 IFCWALL)
    Base Constraint = "Level: 03 Level" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -465. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Core Face: Exterior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 1415. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 5 objects (4 IFCWALLSTANDARDCASE, 1 IFCWALL)
    Base Constraint = "Level: 04 Roof" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -140. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Interior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 04 Roof" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 1750. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 1890. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints: 16 more contents on 26 objects not shown
  Dimensions | properties | on 12 objects (12 IFCMEMBER)
    Area = 0.4875 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.018 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 12 objects (12 IFCMEMBER)
    Area = 0.253500000000001 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 1230. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.00922500000000003 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 4 objects (4 IFCMEMBER)
    Area = 0.2485 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 1205. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.00903749999999999 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 4 objects (4 IFCMEMBER)
    Area = 0.248499999999999 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 1204.99999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.00903749999999996 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 3 objects (3 IFCPLATE)
    Area = 2.82900000000001 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 2300. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0707250000000004 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Width = 1230.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 3 objects (3 IFCPLATE)
    Area = 2.82899999999999 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 2300. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0707249999999999 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Width = 1230. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    Area = 13.9600000000001 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3940.00000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 6.14240000000009 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 67 more contents on 73 objects not shown
  Phasing | properties | on 115 objects (35 IFCWALL, 34 IFCWALLSTANDARDCASE, 32 IFCMEMBER, 8 IFCPLATE)
    Phase Created = "Phase 1" (IFCLABEL)
  Structural | properties | on 71 objects (35 IFCWALL, 34 IFCWALLSTANDARDCASE, 2 IFCCURTAINWALL)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 74 objects (35 IFCWALL, 34 IFCWALLSTANDARDCASE, 5 IFCOPENINGELEMENT) | on 9 type objects
    Roughness = 914.4 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProductRequirements | properties | on 76 objects (35 IFCWALL, 34 IFCWALLSTANDARDCASE, 5 IFCOPENINGELEMENT, 2 IFCCURTAINWALL) | on 10 type objects
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 32 objects (32 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
  Pset_ProductRequirements | properties | on 8 objects (8 IFCPLATE)
    Category = "Curtain Panels" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (2 IFCDOOR)
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "02 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "03 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "04 Roof" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 32 objects (32 IFCMEMBER)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 17 objects (13 IFCWALL, 4 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "00_Külső vázkerámia fal+12 cm hőszigetelés" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 15 objects (8 IFCWALLSTANDARDCASE, 4 IFCWALL, 3 IFCOPENINGELEMENT) | on 1 type object
    Reference = "00_Külső vázkerámia fal 300 mm+vakolat" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 13 objects (13 IFCWALL) | on 1 type object
    Reference = "00_Külső beton fal+2x12 cm szigetelés" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 10 objects (9 IFCWALLSTANDARDCASE, 1 IFCWALL) | on 1 type object
    Reference = "00_Külső vasbeton fal+vakolat" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 8 objects (8 IFCPLATE)
    Reference = "Glazed" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 7 objects (7 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "00_Külső vakolat" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 6 objects (3 IFCWALLSTANDARDCASE, 2 IFCOPENINGELEMENT, 1 IFCWALL) | on 1 type object
    Reference = "00_Külső vázkerámia fal 300 mm+vakolat+szigetelés" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 5 more contents on 10 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 17 objects (13 IFCWALL, 4 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "00_Külső vázkerámia fal+12 cm hőszigetelés" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 13 objects (13 IFCWALL) | on 1 type object
    Reference = "00_Külső beton fal+2x12 cm szigetelés" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 12 objects (8 IFCWALLSTANDARDCASE, 4 IFCWALL) | on 1 type object
    Reference = "00_Külső vázkerámia fal 300 mm+vakolat" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 10 objects (9 IFCWALLSTANDARDCASE, 1 IFCWALL) | on 1 type object
    Reference = "00_Külső vasbeton fal+vakolat" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 7 objects (7 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "00_Külső vakolat" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (3 IFCWALLSTANDARDCASE, 1 IFCWALL) | on 1 type object
    Reference = "00_Külső vázkerámia fal 300 mm+vakolat+szigetelés" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 3 objects (3 IFCWALL) | on 1 type object
    Reference = "00_Külső beton fal 300 mm+vakolat" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 2 objects (2 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "00_Külső vázkerámia fal+2x12 cm hőszigetelés" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 1 more content on 1 objects not shown
  Pset_WallCommon | properties | on 17 objects (13 IFCWALL, 4 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "00_Külső vázkerámia fal+12 cm hőszigetelés" (IFCIDENTIFIER)
    ThermalTransmittance = 0.234799802273851 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 13 objects (13 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "00_Külső beton fal+2x12 cm szigetelés" (IFCIDENTIFIER)
    ThermalTransmittance = 0.177236797437598 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 12 objects (8 IFCWALLSTANDARDCASE, 4 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "00_Külső vázkerámia fal 300 mm+vakolat" (IFCIDENTIFIER)
    ThermalTransmittance = 0.628029969149405 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 10 objects (9 IFCWALLSTANDARDCASE, 1 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "00_Külső vasbeton fal+vakolat" (IFCIDENTIFIER)
    ThermalTransmittance = 14.7490129723632 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 7 objects (7 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "00_Külső vakolat" (IFCIDENTIFIER)
    ThermalTransmittance = 150. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 4 objects (3 IFCWALLSTANDARDCASE, 1 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "00_Külső vázkerámia fal 300 mm+vakolat+szigetelés" (IFCIDENTIFIER)
    ThermalTransmittance = 0.624618844336027 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "00_Külső beton fal 300 mm+vakolat" (IFCIDENTIFIER)
    ThermalTransmittance = 3.33177609785102 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "00_Külső vázkerámia fal+2x12 cm hőszigetelés" (IFCIDENTIFIER)
    ThermalTransmittance = 0.144210461473477 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon: 10 more contents on 1 objects not shown
  Construction | properties | on 2 objects (2 IFCDOOR)
    Swing Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Construction | properties | on 2 type objects
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 440. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 2 type objects
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 320. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "Exterior" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 2 type objects
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 570. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "Exterior" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "Exterior" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Automatically Embed = FALSE (IFCBOOLEAN)
    Function = "Exterior" (IFCIDENTIFIER)
    Join Condition = "Not Defined" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 330. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "Exterior" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 9.99999999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "Exterior" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 2 objects (2 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Függönyfal" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Függönyfal" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 8 objects (8 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Glazed" (IFCIDENTIFIER)
    ThermalTransmittance = 6.7069 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "M_Door-Curtain-Wall-Single-Glass" (IFCIDENTIFIER)
    ThermalTransmittance = 0.5678263 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_MemberCommon | properties | on 12 objects (12 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 2400. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 12 objects (12 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 1230. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 4 objects (4 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 1205. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 4 objects (4 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 1204.99999999999 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Horizontal Grid | properties | on 2 objects (2 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 4 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Horizontal Grid | properties | on 1 type object
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
  Vertical Grid | properties | on 2 objects (2 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 3 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 1 type object
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 3 objects (3 IFCOPENINGELEMENT)
    Reference = "00_Külső vázkerámia fal 300 mm+vakolat" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 2 objects (2 IFCOPENINGELEMENT)
    Reference = "00_Külső vázkerámia fal 300 mm+vakolat+szigetelés" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "02 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "03 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "04 Roof" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 3 (IFCINTEGER)
  Constraints(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Other(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.234799802273851 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 4.25894736842105 (IFCREAL)
    Thermal mass = 426577.2 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.628029969149405 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 1.59228070175439 (IFCREAL)
    Thermal mass = 422520. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.144210461473477 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 6.93430968726163 (IFCREAL)
    Thermal mass = 450206.4 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 14.7490129723632 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 0.0678011472275335 (IFCREAL)
    Thermal mass = 123435. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.177236797437598 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 5.64216920220578 (IFCREAL)
    Thermal mass = 512936.4 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.624618844336027 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 1.6009763539283 (IFCREAL)
    Thermal mass = 442092. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 150. (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 0.00666666666666667 (IFCREAL)
    Thermal mass = 15960. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.337062720734191 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 2.9668068833652 (IFCREAL)
    Thermal mass = 489307.2 (IFCREAL)
  Analytical Properties: 1 more content on 0 objects not shown
  Graphics | properties | on 9 type objects
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Materials and Finishes | properties | on 4 type objects
    Structural Material = "02_Porotherm 30 N+F tégla" (IFCLABEL)
  Materials and Finishes | properties | on 4 type objects
    Structural Material = "02_Vasbeton, helyszíni C40/55" (IFCLABEL)

Other addresses and roles
  2 x postal address: "Enter address here", "Boston", "MA"