IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "0001"
Time stamp: "2021-05-09T13:44:10"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190327_2315(x64) - Exporter 20.0.0.377 - Alternate UI 20.0.0.377"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "jozsef.etlinger" of Organization (no name given)
  Owner history of Person "jozsef.etlinger" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1620559188 (2021-05-09T11:19:48Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "03 Level" | long name "03 Level" | object type "Level:8mm Head" | elevation 12000.
        contains 16 elements
          16 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "PCSQS-22-ULO-FH-LED-80-2500-35" | object type "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall:PCSQS-22-ULO-FH-LED-80-2500-35" | names: "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall:PCSQS-22-ULO-FH-LED-80-2500-35:633970", "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall:PCSQS-22-ULO-FH-LED-80-2500-35:672535", "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall:PCSQS-22-ULO-FH-LED-80-2500-35:672585" (+13 more) | material: materials ("Lumenwerx Standard White", "Lumenwerx ULO Optic") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
      IFCBUILDINGSTOREY "04 Roof" | long name "04 Roof" | object type "Level:8mm Head" | elevation 16000.
        contains 125 elements
          65 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "PCSQS-22-ULO-FH-LED-80-2500-35" | object type "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall:PCSQS-22-ULO-FH-LED-80-2500-35" | names: "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall:PCSQS-22-ULO-FH-LED-80-2500-35:631692", "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall:PCSQS-22-ULO-FH-LED-80-2500-35:632116", "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall:PCSQS-22-ULO-FH-LED-80-2500-35:632281" (+62 more) | material: materials ("Lumenwerx Standard White", "Lumenwerx ULO Optic") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          60 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "PCSQS-22-ULO-FH-LED-80-2500-35" | object type "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall:PCSQS-22-ULO-FH-LED-80-2500-35" | names: "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall:PCSQS-22-ULO-FH-LED-80-2500-35:633364", "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall:PCSQS-22-ULO-FH-LED-80-2500-35:633366", "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall:PCSQS-22-ULO-FH-LED-80-2500-35:633842" (+57 more) | material: materials ("Lumenwerx Standard White", "Lumenwerx ULO Optic") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions

Types
  IFCLIGHTFIXTURETYPE "PCSQS-22-ULO-FH-LED-80-2500-35" | 81 occurrences | material: materials ("Lumenwerx Standard White", "Lumenwerx ULO Optic") | property sets: Constraints, Dimensions, Electrical, Electrical - Loads, Electrical Engineering, General
  IFCLIGHTFIXTURETYPE "PCSQS-22-ULO-FH-LED-80-2500-35" | 60 occurrences | material: materials ("Lumenwerx Standard White", "Lumenwerx ULO Optic") | property sets: Constraints, Dimensions, Electrical, Electrical - Loads, Electrical Engineering, General

Property sets
  Other(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 141 objects (141 IFCFLOWTERMINAL)
    Category = "Lighting Fixtures" (IFCLABEL)
    Family = "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall: PCSQS-22-ULO-FH-LED-80-2500-35" (IFCLABEL)
    Family and Type = "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall: PCSQS-22-ULO-FH-LED-80-2500-35" (IFCLABEL)
    Type = "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall: PCSQS-22-ULO-FH-LED-80-2500-35" (IFCLABEL)
    Type Id = "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall: PCSQS-22-ULO-FH-LED-80-2500-35" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 2 type objects
    Category = "Lighting Fixtures" (IFCLABEL)
    Family Name = "Lighting_Ceiling-Mounted_LumenWerx_Pop-Core-Square-Surface-Wall" (IFCTEXT)
  Identity Data(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Graphics(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Comments = "Világítás" (IFCTEXT)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Comments = "Világítás" (IFCTEXT)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Comments = "Világítás" (IFCTEXT)
    Mark = "3" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Comments = "Világítás" (IFCTEXT)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Comments = "Világítás" (IFCTEXT)
    Mark = "5" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Comments = "Világítás" (IFCTEXT)
    Mark = "6" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Comments = "Világítás" (IFCTEXT)
    Mark = "7" (IFCTEXT)
  Identity Data: 137 more contents on 136 objects not shown
  Constraints(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 141 objects (141 IFCFLOWTERMINAL)
    Reference = "PCSQS-22-ULO-FH-LED-80-2500-35" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 141 objects (141 IFCFLOWTERMINAL)
    Manufacturer = "Lumenwerx" (IFCLABEL)
  Pset_ProductRequirements | properties | on 141 objects (141 IFCFLOWTERMINAL)
    Category = "Lighting Fixtures" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "03 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "04 Roof" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 141 objects (141 IFCFLOWTERMINAL)
    Reference = "PCSQS-22-ULO-FH-LED-80-2500-35" (IFCIDENTIFIER)
  Constraints | properties | on 18 objects (18 IFCFLOWTERMINAL)
    Elevation from Level = -340.000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Floor : Vasbeton 200mm" (IFCTEXT)
    Level = "Level: 04 Roof" (IFCLABEL)
    Schedule Level = "Level: 04 Roof" (IFCLABEL)
  Constraints | properties | on 18 objects (18 IFCFLOWTERMINAL)
    Elevation from Level = -12340. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Floor : Vasbeton 200mm" (IFCTEXT)
    Level = "Level: 04 Roof" (IFCLABEL)
    Schedule Level = "Level: 04 Roof" (IFCLABEL)
  Constraints | properties | on 16 objects (16 IFCFLOWTERMINAL)
    Elevation from Level = -8340. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Floor : Vasbeton 200mm" (IFCTEXT)
    Level = "Level: 04 Roof" (IFCLABEL)
    Schedule Level = "Level: 04 Roof" (IFCLABEL)
  Constraints | properties | on 16 objects (16 IFCFLOWTERMINAL)
    Elevation from Level = -4340. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Floor : Vasbeton 200mm" (IFCTEXT)
    Level = "Level: 04 Roof" (IFCLABEL)
    Schedule Level = "Level: 04 Roof" (IFCLABEL)
  Constraints | properties | on 8 objects (8 IFCFLOWTERMINAL)
    Elevation from Level = -9400. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Compound Ceiling : Álmennyezet 3" (IFCTEXT)
    Level = "Level: 04 Roof" (IFCLABEL)
    Schedule Level = "Level: 04 Roof" (IFCLABEL)
  Constraints | properties | on 8 objects (8 IFCFLOWTERMINAL)
    Elevation from Level = -5400. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Compound Ceiling : Álmennyezet 3" (IFCTEXT)
    Level = "Level: 04 Roof" (IFCLABEL)
    Schedule Level = "Level: 04 Roof" (IFCLABEL)
  Constraints | properties | on 8 objects (8 IFCFLOWTERMINAL)
    Elevation from Level = -1400. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Compound Ceiling : Álmennyezet 3" (IFCTEXT)
    Level = "Level: 04 Roof" (IFCLABEL)
    Schedule Level = "Level: 04 Roof" (IFCLABEL)
  Constraints | properties | on 6 objects (6 IFCFLOWTERMINAL)
    Elevation from Level = -9400. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Compound Ceiling : Álmennyezet 2" (IFCTEXT)
    Level = "Level: 04 Roof" (IFCLABEL)
    Schedule Level = "Level: 04 Roof" (IFCLABEL)
  Constraints: 15 more contents on 45 objects not shown
  Dimensions | properties | on 81 objects (81 IFCFLOWTERMINAL)
    Area = 1.03915793824753 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00328582139322307 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 60 objects (60 IFCFLOWTERMINAL)
    Area = 1.03915793824753 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00328582139322308 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 type objects
    Diffuser Height = 63.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Diffuser Length = 581.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Diffuser Width = 581.025 (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Circuiting | properties | on 141 objects (141 IFCFLOWTERMINAL)
    Electrical Data = "120 V/1-0 VA" (IFCTEXT)
  Electrical - Loads | properties | on 141 objects (141 IFCFLOWTERMINAL)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Electrical - Loads | properties | on 2 type objects
    Apparent Load = 0. (IFCPOWERMEASURE) [WATT]
  Phasing | properties | on 141 objects (141 IFCFLOWTERMINAL)
    Phase Created = "Phase 1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "03 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "04 Roof" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 2 (IFCINTEGER)
  Electrical | properties | on 2 type objects
    120 Volts = TRUE (IFCBOOLEAN)
    277 Volts = FALSE (IFCBOOLEAN)
    347 Volts = FALSE (IFCBOOLEAN)
    Lamp = "LED" (IFCTEXT)
    UNV 120 Volts-277 Volts = FALSE (IFCBOOLEAN)
  Electrical Engineering | properties | on 2 type objects
    Voltage = 120. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  General | properties | on 2 type objects
    Edition number = 1 (IFCINTEGER)
  Materials and Finishes | properties | on 2 type objects
    Finish = "Lumenwerx Standard White" (IFCLABEL)
    Optics = "Lumenwerx ULO Optic" (IFCLABEL)
  Photometrics | properties | on 2 type objects
    Color Filter = 16777215 (IFCINTEGER)
    Color Temperature = 3500. (IFCREAL) [KELVIN]
    Dimming Lamp Color Temperature Shift = "<None>" (IFCIDENTIFIER)
    Efficacy = 148.541963750594 (IFCREAL) [derived "Luminous Efficacy"]
    Emit Shape Visible in Rendering = FALSE (IFCBOOLEAN)
    Emit from Circle Diameter = 609.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Illuminance = 11.8205938937421 (IFCILLUMINANCEMEASURE) [LUX]
    Initial Color = 0 (IFCINTEGER)
    Initial Color Temperature = 3200. (IFCREAL) [KELVIN]
    Initial Intensity = 0 (IFCINTEGER)
    Light Loss Factor = 0 (IFCINTEGER)
    Light Source Definition (family) = "Circle+Photometric Web" (IFCTEXT)
    Luminous Flux = 1380. (IFCLUMINOUSFLUXMEASURE) [LUMEN]
    Luminous Intensity = 109.816910733408 (IFCLUMINOUSINTENSITYMEASURE) [CANDELA]
    Photometric Web File = "PCSQD-22-ULO-LED-80-2500-35" (IFCTEXT)
    Tilt Angle = -90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Total Light Loss Factor = 1. (IFCREAL)
    Wattage = 9.290304 (IFCPOWERMEASURE) [WATT]
  Text | properties | on 2 type objects
    Link to IES File = "http://www.lumenwerx.com/product?downloads&product_line[]=popcolor&byfolder[]=photometry" (IFCTEXT)
    Link to Product Page = "http://www.lumenwerx.com/product?category=POPCOLOR" (IFCTEXT)
    Lumen Package = "2500 lm/ft" (IFCTEXT)
    Luminaire ID = "PCSQS" (IFCTEXT)

Other addresses and roles
  2 x postal address: "Enter address here", "Boston", "MA"