IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "0001"
Time stamp: "2021-05-09T13:42:45"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190327_2315(x64) - Exporter 20.0.0.377 - Alternate UI 20.0.0.377"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "jozsef.etlinger" of Organization (no name given)
  Owner history of Person "jozsef.etlinger" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1620559188 (2021-05-09T11:19:48Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "00 Ground level" | long name "00 Ground level" | object type "Level:8mm Head" | elevation 0.
        contains 3 elements
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Feketeacél cső" | object type "Pipe Types:Feketeacél cső" | names: "Pipe Types:Feketeacél cső:623064" | property sets: Constraints, Dimensions, Insulation, Mechanical, Mechanical - Flow, Other
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "magi_pipe_fe_tee_centric_90_001" | object type "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001" | names: "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001:623099" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Coupling - Generic:Standard" | names: "M_Coupling - Generic:Standard:623131" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
      IFCBUILDINGSTOREY "01 Level" | long name "01 Level" | object type "Level:8mm Head" | elevation 4000.
        contains 8 elements
          6 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Feketeacél cső" | object type "Pipe Types:Feketeacél cső" | names: "Pipe Types:Feketeacél cső:622873", "Pipe Types:Feketeacél cső:622995", "Pipe Types:Feketeacél cső:623052" (+3 more) | property sets: Constraints, Dimensions, Identity Data, Insulation, Mechanical, Mechanical - Flow
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "magi_pipe_fe_tee_centric_90_001" | object type "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001" | names: "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001:623051" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Coupling - Generic:Standard" | names: "M_Coupling - Generic:Standard:623145" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
      IFCBUILDINGSTOREY "02 Level" | long name "02 Level" | object type "Level:8mm Head" | elevation 8000.
        contains 3 elements
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Feketeacél cső" | object type "Pipe Types:Feketeacél cső" | names: "Pipe Types:Feketeacél cső:623068" | property sets: Constraints, Dimensions, Insulation, Mechanical, Mechanical - Flow, Other
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "magi_pipe_fe_tee_centric_90_001" | object type "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001" | names: "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001:623103" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Coupling - Generic:Standard" | names: "M_Coupling - Generic:Standard:623158" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
      IFCBUILDINGSTOREY "03 Level" | long name "03 Level" | object type "Level:8mm Head" | elevation 12000.
        contains 3 elements
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Feketeacél cső" | object type "Pipe Types:Feketeacél cső" | names: "Pipe Types:Feketeacél cső:623072" | property sets: Constraints, Dimensions, Insulation, Mechanical, Mechanical - Flow, Other
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "magi_pipe_fe_tee_centric_90_001" | object type "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001" | names: "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001:623109" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Coupling - Generic:Standard" | names: "M_Coupling - Generic:Standard:623171" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
      IFCBUILDINGSTOREY "04 Roof" | long name "04 Roof" | object type "Level:8mm Head" | elevation 16000.
        contains 3 elements
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Feketeacél cső" | object type "Pipe Types:Feketeacél cső" | names: "Pipe Types:Feketeacél cső:623076" | property sets: Constraints, Dimensions, Insulation, Mechanical, Mechanical - Flow, Other
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "magi_pipe_fe_elbow_short_001" | object type "magi_pipe_fe_elbow_short_001:magi_pipe_fe_elbow_short_001" | names: "magi_pipe_fe_elbow_short_001:magi_pipe_fe_elbow_short_001:623115" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Coupling - Generic:Standard" | names: "M_Coupling - Generic:Standard:623184" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics

Types
  IFCPIPESEGMENTTYPE "Pipe Types:Feketeacél cső" | 10 occurrences | property sets: Identity Data, Other
  IFCPIPEFITTINGTYPE "magi_pipe_fe_tee_centric_90_001" | 4 occurrences | property sets: Constraints, Dimensions, Identity Data, Mechanical, Other
  IFCPIPEFITTINGTYPE "Standard" | 5 occurrences | property sets: Constraints, Identity Data, Mechanical, Other
  IFCPIPEFITTINGTYPE "magi_pipe_fe_elbow_short_001" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Mechanical, Other

Property sets
  Other | properties | on 20 objects (20 IFCFLOWSEGMENT)
    Category = "Pipes" (IFCLABEL)
    Family = "Pipe Types: Feketeacél cső" (IFCLABEL)
    Family and Type = "Pipe Types: Feketeacél cső" (IFCLABEL)
    Type = "Pipe Types: Feketeacél cső" (IFCLABEL)
    Type Id = "Pipe Types: Feketeacél cső" (IFCLABEL)
  Other | properties | on 5 objects (5 IFCFLOWFITTING)
    Category = "Pipe Fittings" (IFCLABEL)
    Family = "M_Coupling - Generic: Standard" (IFCLABEL)
    Family and Type = "M_Coupling - Generic: Standard" (IFCLABEL)
    Fitting Outside Radius = 56.5875 (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "M_Coupling - Generic: Standard" (IFCLABEL)
    Type Id = "M_Coupling - Generic: Standard" (IFCLABEL)
  Other | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 4 objects (4 IFCFLOWFITTING)
    Category = "Pipe Fittings" (IFCLABEL)
    Family = "magi_pipe_fe_tee_centric_90_001: magi_pipe_fe_tee_centric_90_001" (IFCLABEL)
    Family and Type = "magi_pipe_fe_tee_centric_90_001: magi_pipe_fe_tee_centric_90_001" (IFCLABEL)
    Type = "magi_pipe_fe_tee_centric_90_001: magi_pipe_fe_tee_centric_90_001" (IFCLABEL)
    Type Id = "magi_pipe_fe_tee_centric_90_001: magi_pipe_fe_tee_centric_90_001" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWFITTING)
    Category = "Pipe Fittings" (IFCLABEL)
    Family = "magi_pipe_fe_elbow_short_001: magi_pipe_fe_elbow_short_001" (IFCLABEL)
    Family and Type = "magi_pipe_fe_elbow_short_001: magi_pipe_fe_elbow_short_001" (IFCLABEL)
    Type = "magi_pipe_fe_elbow_short_001: magi_pipe_fe_elbow_short_001" (IFCLABEL)
    Type Id = "magi_pipe_fe_elbow_short_001: magi_pipe_fe_elbow_short_001" (IFCLABEL)
  Other | properties | on 1 object (1 IFCSYSTEM)
    Category = "Piping Systems" (IFCLABEL)
    Family = "Piping System: D4010.10.001-Gerincvezeték" (IFCLABEL)
    Family and Type = "Piping System: D4010.10.001-Gerincvezeték" (IFCLABEL)
    Type = "Piping System: D4010.10.001-Gerincvezeték" (IFCLABEL)
    Type Id = "Piping System: D4010.10.001-Gerincvezeték" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Pipes" (IFCLABEL)
    Family Name = "Pipe Types" (IFCTEXT)
  Other: 3 more contents on 0 objects not shown
  Constraints | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Bottom Elevation = 9110. (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 9110. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 12890. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 01 Level" (IFCLABEL)
    Start Middle Elevation = 12890. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 12890. (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Bottom Elevation = 945. (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 01 Level" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 1055. (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 2 objects (2 IFCFLOWFITTING)
    Elevation from Level = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: 01 Level" (IFCLABEL)
  Constraints | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Bottom Elevation = -4000. (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = -4000. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = -3110. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 01 Level" (IFCLABEL)
    Start Middle Elevation = -3110. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = -3110. (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Bottom Elevation = 945.000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 00 Ground level" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 1055. (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Bottom Elevation = 945.000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 02 Level" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 1055. (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Bottom Elevation = 945. (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 03 Level" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 1055. (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Bottom Elevation = 945. (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 04 Roof" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 1055. (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints: 13 more contents on 19 objects not shown
  Dimensions | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Inside Diameter = 95.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 3780. (IFCLENGTHMEASURE) [MILLI METRE]
    Outside Diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "110 mmø" (IFCTEXT)
  Dimensions | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Inside Diameter = 95.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 190.972824049356 (IFCLENGTHMEASURE) [MILLI METRE]
    Outside Diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "110 mmø" (IFCTEXT)
  Dimensions | properties | on 5 objects (5 IFCFLOWFITTING)
    Fitting Outside Diameter = 113.175 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 56.5875 (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Size = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Size = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Radius = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "110 mmø-110 mmø" (IFCTEXT)
    Tick Size = 45.27 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.000569233933504018 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 4 objects (4 IFCFLOWFITTING)
    BranchL1 = 82.5 (IFCLENGTHMEASURE) [MILLI METRE]
    MainL = 220. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Size = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Size = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Rout1 = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Rout1ToMC_R1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rout1_Ins = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Rout3 = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Rout3ToMC_R3 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rout3_Ins = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "110 mmø-110 mmø-110 mmø" (IFCTEXT)
    Visibilty_Ins = FALSE (IFCBOOLEAN)
    Volume = 0.00243098413509303 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    W2D_1 = 44. (IFCLENGTHMEASURE) [MILLI METRE]
    W2D_3 = 44. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Inside Diameter = 95.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 890.000000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    Outside Diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "110 mmø" (IFCTEXT)
  Dimensions | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Inside Diameter = 95.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 163.472824049353 (IFCLENGTHMEASURE) [MILLI METRE]
    Outside Diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "110 mmø" (IFCTEXT)
  Dimensions | properties | on 1 object (1 IFCFLOWFITTING)
    Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Angle_list = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    L = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    MC_RtoRout = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Size = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Size = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Rout = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Rout_Ins = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "110 mmø-110 mmø" (IFCTEXT)
    Visibilty_Ins = FALSE (IFCBOOLEAN)
    Volume = 0.00164200609072829 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    W2D = 44. (IFCLENGTHMEASURE) [MILLI METRE]
    rc = 110. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions: 1 more content on 0 objects not shown
  Identity Data | properties | on 10 objects (10 IFCFLOWSEGMENT)
    Comments = "Padlófűtés" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "00 Ground level" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "01 Level" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "02 Level" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "03 Level" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "04 Roof" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Description = "Feketeacél" (IFCTEXT)
    Type Comments = "DN" (IFCTEXT)
    Type Name = "Feketeacél cső" (IFCTEXT)
    magiUserCode = "FE" (IFCTEXT)
  Identity Data: 3 more contents on 0 objects not shown
  Insulation | properties | on 20 objects (20 IFCFLOWSEGMENT)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "110 mmø" (IFCTEXT)
  Insulation | properties | on 6 objects (6 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "110 mmø-110 mmø" (IFCTEXT)
  Insulation | properties | on 4 objects (4 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "110 mmø-110 mmø-110 mmø" (IFCTEXT)
  Mechanical | properties | on 5 objects (5 IFCFLOWFITTING)
    Loss Method = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Fire Protection Wet" (IFCTEXT)
    System Name = "D4010.10.001-Gerincvezeték 1" (IFCTEXT)
    System Type = "Piping System: D4010.10.001-Gerincvezeték" (IFCLABEL)
  Mechanical | properties | on 4 objects (4 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Method = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
    MC_R1 = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    MC_R3 = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Fire Protection Wet" (IFCTEXT)
    System Name = "D4010.10.001-Gerincvezeték 1" (IFCTEXT)
    System Type = "Piping System: D4010.10.001-Gerincvezeték" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 1.30627422536263 (IFCAREAMEASURE) [SQUARE_METRE]
    Connection Type = "Generic" (IFCTEXT)
    Diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Invert Elevation = 13110. (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "Feketeacél cső" (IFCLABEL)
    Pipe Segment = "Feketeacél cső" (IFCLABEL)
    Roughness = 0.0450000017881393 (IFCLENGTHMEASURE) [MILLI METRE]
    Schedule/Type = "Pipe Schedule Types: Schedule 40" (IFCLABEL)
    Section = 36 (IFCINTEGER)
    Segment Description = "Feketeacél" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Fire Protection Wet" (IFCTEXT)
    System Name = "D4010.10.001-Gerincvezeték 1" (IFCTEXT)
    System Type = "Piping System: D4010.10.001-Gerincvezeték" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 0.0659954703175626 (IFCAREAMEASURE) [SQUARE_METRE]
    Connection Type = "Generic" (IFCTEXT)
    Diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Invert Elevation = 4952.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "Feketeacél cső" (IFCLABEL)
    Pipe Segment = "Feketeacél cső" (IFCLABEL)
    Roughness = 0.0450000017881393 (IFCLENGTHMEASURE) [MILLI METRE]
    Schedule/Type = "Pipe Schedule Types: Schedule 40" (IFCLABEL)
    Section = 1 (IFCINTEGER)
    Segment Description = "Feketeacél" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Fire Protection Wet" (IFCTEXT)
    System Name = "D4010.10.001-Gerincvezeték 1" (IFCTEXT)
    System Type = "Piping System: D4010.10.001-Gerincvezeték" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 0.307561920786441 (IFCAREAMEASURE) [SQUARE_METRE]
    Connection Type = "Generic" (IFCTEXT)
    Diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Invert Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "Feketeacél cső" (IFCLABEL)
    Pipe Segment = "Feketeacél cső" (IFCLABEL)
    Roughness = 0.0450000017881393 (IFCLENGTHMEASURE) [MILLI METRE]
    Schedule/Type = "Pipe Schedule Types: Schedule 40" (IFCLABEL)
    Section = 31 (IFCINTEGER)
    Segment Description = "Feketeacél" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Fire Protection Wet" (IFCTEXT)
    System Name = "D4010.10.001-Gerincvezeték 1" (IFCTEXT)
    System Type = "Piping System: D4010.10.001-Gerincvezeték" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 0.0659954703175626 (IFCAREAMEASURE) [SQUARE_METRE]
    Connection Type = "Generic" (IFCTEXT)
    Diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Invert Elevation = 952.100000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "Feketeacél cső" (IFCLABEL)
    Pipe Segment = "Feketeacél cső" (IFCLABEL)
    Roughness = 0.0450000017881393 (IFCLENGTHMEASURE) [MILLI METRE]
    Schedule/Type = "Pipe Schedule Types: Schedule 40" (IFCLABEL)
    Section = 33 (IFCINTEGER)
    Segment Description = "Feketeacél" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Fire Protection Wet" (IFCTEXT)
    System Name = "D4010.10.001-Gerincvezeték 1" (IFCTEXT)
    System Type = "Piping System: D4010.10.001-Gerincvezeték" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 0.0659954703175626 (IFCAREAMEASURE) [SQUARE_METRE]
    Connection Type = "Generic" (IFCTEXT)
    Diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Invert Elevation = 8952.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "Feketeacél cső" (IFCLABEL)
    Pipe Segment = "Feketeacél cső" (IFCLABEL)
    Roughness = 0.0450000017881393 (IFCLENGTHMEASURE) [MILLI METRE]
    Schedule/Type = "Pipe Schedule Types: Schedule 40" (IFCLABEL)
    Section = 35 (IFCINTEGER)
    Segment Description = "Feketeacél" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Fire Protection Wet" (IFCTEXT)
    System Name = "D4010.10.001-Gerincvezeték 1" (IFCTEXT)
    System Type = "Piping System: D4010.10.001-Gerincvezeték" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 0.0659954703175626 (IFCAREAMEASURE) [SQUARE_METRE]
    Connection Type = "Generic" (IFCTEXT)
    Diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Invert Elevation = 12952.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "Feketeacél cső" (IFCLABEL)
    Pipe Segment = "Feketeacél cső" (IFCLABEL)
    Roughness = 0.0450000017881393 (IFCLENGTHMEASURE) [MILLI METRE]
    Schedule/Type = "Pipe Schedule Types: Schedule 40" (IFCLABEL)
    Section = 37 (IFCINTEGER)
    Segment Description = "Feketeacél" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Fire Protection Wet" (IFCTEXT)
    System Name = "D4010.10.001-Gerincvezeték 1" (IFCTEXT)
    System Type = "Piping System: D4010.10.001-Gerincvezeték" (IFCLABEL)
  Mechanical: 8 more contents on 10 objects not shown
  Mechanical - Flow | properties | on 20 objects (20 IFCFLOWSEGMENT)
    Relative Roughness = 0.000469728619917947 (IFCREAL)
  Mechanical - Flow | properties | on 4 objects (4 IFCFLOWFITTING)
    Pressure Drop = 0. (IFCPRESSUREMEASURE) [PASCAL]
  Phasing | properties | on 30 objects (20 IFCFLOWSEGMENT, 10 IFCFLOWFITTING)
    Phase Created = "Phase 1" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 10 objects (10 IFCFLOWSEGMENT)
    Reference = "Feketeacél cső" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 5 objects (5 IFCFLOWFITTING)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 4 objects (4 IFCFLOWFITTING)
    Reference = "magi_pipe_fe_tee_centric_90_001" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWFITTING)
    Reference = "magi_pipe_fe_elbow_short_001" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 10 objects (10 IFCFLOWSEGMENT)
    Roughness = 0.0450000017881393 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Length = 3780. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Length = 190.972824049356 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 890.000000000002 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 163.472824049353 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 13110. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 3780. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 4952.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 190.972824049356 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 890.000000000002 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 952.100000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 190.972824049356 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 8952.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 190.972824049356 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 12952.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 190.972824049356 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 16952.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 163.472824049353 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 1110. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 3780. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment: 2 more contents on 2 objects not shown
  Pset_ProductRequirements | properties | on 10 objects (10 IFCFLOWSEGMENT)
    Category = "Pipes" (IFCLABEL)
  Pset_ProductRequirements | properties | on 10 objects (10 IFCFLOWFITTING)
    Category = "Pipe Fittings" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "00 Ground level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "01 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "02 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "03 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "04 Roof" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 10 objects (10 IFCFLOWSEGMENT)
    Reference = "Feketeacél cső" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCFLOWFITTING)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCFLOWFITTING)
    Reference = "magi_pipe_fe_tee_centric_90_001" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFLOWFITTING)
    Reference = "magi_pipe_fe_elbow_short_001" (IFCIDENTIFIER)
  Graphics | properties | on 10 objects (10 IFCFLOWFITTING)
    Use Annotation Scale = FALSE (IFCBOOLEAN)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "00 Ground level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "01 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "02 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "03 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "04 Roof" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 5 (IFCINTEGER)
  Constraints(Type) | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Other(Type) | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)

Other addresses and roles
  2 x postal address: "Enter address here", "Boston", "MA"