IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2020-03-05T14:53:27"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190225_1515(x64) - Exporter 19.1.0.0 - Alternate UI 19.1.0.0"
Application: "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)"

People and organizations
  Person "info@bimprove.eu" of Organization (no name given)
  Owner history of Person "info@bimprove.eu" of Organization (no name given) | application "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)" | change NOCHANGE | created 1583072663 (2020-03-01T14:24:23Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Surface:287499" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "T.O. Slab" | long name "T.O. Slab" | object type "Level:8mm Head" | elevation -4000.
        contains 2 elements
          2 x IFCRAMP | object type "Ramp:Ramp 1" | names: "Ramp:Ramp 1:298866", "Ramp:Ramp 1:299088" | parts: 2 IFCRAMPFLIGHT | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RampCommon
      IFCBUILDINGSTOREY "T.O. Fnd. Wall" | long name "T.O. Fnd. Wall" | object type "Level:8mm Head" | elevation -300.
        contains 1 element
          1 x IFCRAMP | object type "Ramp:Ramp 1" | names: "Ramp:Ramp 1:299055" | parts: 1 IFCRAMPFLIGHT | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RampCommon
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | object type "Level:8mm Head" | elevation 0.
        contains 69 elements
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" | object type "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" | names: "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat:288491", "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat:288493", "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat:288494" (+1 more) | material: layers "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" ("Concrete Masonry Units (1)" 100., "Air" 50., "Air Infiltration Barrier" 25., "Metal Stud Layer" 100.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" | object type "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" | names: "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat:288492" | material: layers "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" ("Concrete Masonry Units (1)" 100., "Air" 50., "Air Infiltration Barrier" 25., "Metal Stud Layer" 100.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton födém, úsztatott beton, parketta" | object type "Floor:Vasbeton födém, úsztatott beton, parketta" | FLOOR | names: "Floor:Vasbeton födém, úsztatott beton, parketta:288774" | material: layers "Floor:Vasbeton födém, úsztatott beton, parketta" ("Default Floor" 20., "Default Floor" 50., "Default Floor" 30., "Default Floor" 200., "Default Floor" 10.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Interior - 126mm Partition (2-hr)" | object type "Basic Wall:Interior - 126mm Partition (2-hr)" | names: "Basic Wall:Interior - 126mm Partition (2-hr):290475", "Basic Wall:Interior - 126mm Partition (2-hr):290522", "Basic Wall:Interior - 126mm Partition (2-hr):290573" (+2 more) | material: layers "Basic Wall:Interior - 126mm Partition (2-hr)" ("Gypsum Wall Board" 16., "Gypsum Wall Board" 16., "Metal Stud Layer" 64., "Gypsum Wall Board" 16., "Gypsum Wall Board" 16.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | names: "M_Single-Flush:0915 x 2134mm:290838" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | names: "M_Single-Flush:0915 x 2134mm:290867" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "0762 x 2134mm" | object type "M_Single-Flush:0762 x 2134mm" | names: "M_Single-Flush:0762 x 2134mm:290934", "M_Single-Flush:0762 x 2134mm:290956" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | names: "M_Single-Flush:0915 x 2134mm:291025" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          4 x IFCWINDOW | type IFCWINDOWSTYLE "1200 x 1500mm" | object type "M_Window-Casement-Double:1200 x 1500mm" | names: "M_Window-Casement-Double:1200 x 1500mm:291112", "M_Window-Casement-Double:1200 x 1500mm:291152", "M_Window-Casement-Double:1200 x 1500mm:291367" (+1 more) | material: materials ("Wood - Stained", "Glass") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon
          6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Muntin Pattern_2x2" | object type "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2" | names: "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2:291114", "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2:291154", "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2:291228" (+3 more) | material: materials ("Clad - White", "Wood - Stained") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Muntin Pattern_2x2" | object type "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2" | names: "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2:291115", "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2:291155", "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2:291227" (+3 more) | material: materials ("Clad - White", "Wood - Stained") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "with Sill" | object type "M_Trim-Window-Exterior-Flat:with Sill" | names: "M_Trim-Window-Exterior-Flat:with Sill:291116", "M_Trim-Window-Exterior-Flat:with Sill:291156", "M_Trim-Window-Exterior-Flat:with Sill:291371" (+1 more) | material: "Clad - White" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Picture Frame" | object type "M_Trim-Window-Interior-Flat:Picture Frame" | names: "M_Trim-Window-Interior-Flat:Picture Frame:291117", "M_Trim-Window-Interior-Flat:Picture Frame:291157", "M_Trim-Window-Interior-Flat:Picture Frame:291372" (+1 more) | material: "Wood - Stained" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          2 x IFCWINDOW | type IFCWINDOWSTYLE "1200 x 1500mm" | object type "M_Window-Casement-Double:1200 x 1500mm" | names: "M_Window-Casement-Double:1200 x 1500mm:291226", "M_Window-Casement-Double:1200 x 1500mm:291231" | material: materials ("Wood - Stained", "Glass") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "with Sill" | object type "M_Trim-Window-Exterior-Flat:with Sill" | names: "M_Trim-Window-Exterior-Flat:with Sill:291229", "M_Trim-Window-Exterior-Flat:with Sill:291234" | material: "Clad - White" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Picture Frame" | object type "M_Trim-Window-Interior-Flat:Picture Frame" | names: "M_Trim-Window-Interior-Flat:Picture Frame:291230", "M_Trim-Window-Interior-Flat:Picture Frame:291235" | material: "Wood - Stained" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCSTAIR | object type "Cast-In-Place Stair:Monolithic Stair" | names: "Cast-In-Place Stair:Stair:291427" | parts: 1 IFCSTAIRFLIGHT | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_StairCommon
          2 x IFCFLOWTERMINAL | object type "M_Sink Kitchen-Single:760 x 535mm" | names: "M_Sink Kitchen-Single:760 x 535mm:294904", "M_Sink Kitchen-Single:760 x 535mm:294965" | material: "Steel, Polished" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCFLOWTERMINAL | object type "M_Toilet-Domestic-3D:M_Toilet-Domestic-3D" | names: "M_Toilet-Domestic-3D:M_Toilet-Domestic-3D:296543" | material: materials ("Porcelain, Linen", "Laminate, Linen, Matte") | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "1525mm Diameter" | object type "M_Table-Dining Round w Chairs:1525mm Diameter" | names: "M_Table-Dining Round w Chairs:1525mm Diameter:297867" | material: materials ("Pine", "Laminate, Linen, Matte") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff
          6 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "M_Chair-Breuer" | object type "M_Chair-Breuer:M_Chair-Breuer" | names: "M_Chair-Breuer:M_Chair-Breuer:297868", "M_Chair-Breuer:M_Chair-Breuer:297869", "M_Chair-Breuer:M_Chair-Breuer:297870" (+3 more) | material: materials ("Textile - Bamboo Weave", "Steel, Chrome Plated") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff
          2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "1525 x 2007mm - Queen" | object type "M_Bed-Box:1525 x 2007mm - Queen" | names: "M_Bed-Box:1525 x 2007mm - Queen:298651", "M_Bed-Box:1525 x 2007mm - Queen:298700" | material: materials ("Linen, White", "Birch") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Storefront" | object type "Curtain Wall:Storefront" | names: "Curtain Wall:Storefront:299780" | parts: 63 IFCMEMBER, 25 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCSITE | object type "M_Truck - Pick-Up:Pick-Up Truck" | names: "M_Truck - Pick-Up:Pick-Up Truck:301646" | material: materials ("Steel", "Metal - Paint Finish - Blue, Sky", "Rubber - Black") | property sets: Pset_ProductRequirements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "8,5" | object type "M_Chimney:8,5" | names: "M_Chimney:8,5:302363" | material: "Pine" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Largetooth Aspen - 7.6 Meters" | object type "M_RPC Tree - Deciduous:Largetooth Aspen - 7.6 Meters" | names: "M_RPC Tree - Deciduous:Largetooth Aspen - 7.6 Meters:307336" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Lombardy Poplar - 12.2 Meters" | object type "M_RPC Tree - Deciduous:Lombardy Poplar - 12.2 Meters" | names: "M_RPC Tree - Deciduous:Lombardy Poplar - 12.2 Meters:307381" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Red Ash - 7.6 Meters" | object type "M_RPC Tree - Deciduous:Red Ash - 7.6 Meters" | names: "M_RPC Tree - Deciduous:Red Ash - 7.6 Meters:307757", "M_RPC Tree - Deciduous:Red Ash - 7.6 Meters:308159", "M_RPC Tree - Deciduous:Red Ash - 7.6 Meters:308240" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "8,5" | object type "M_Chimney:8,5" | names: "M_Chimney:8,5:310027" | material: "Pine" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "535 x 910 x 810mm" | object type "M_Boiler:535 x 910 x 810mm" | names: "M_Boiler:535 x 910 x 810mm:311021" | material: "Steel, Paint Finish, Ivory, Glossy" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 3000.
        contains 59 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Vasbeton födém, úsztatott beton, parketta" | object type "Floor:Vasbeton födém, úsztatott beton, parketta" | FLOOR | names: "Floor:Vasbeton födém, úsztatott beton, parketta:289044" | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          4 x IFCWALL | type IFCWALLTYPE "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" | object type "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" | names: "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat:289580", "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat:289581", "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat:289582" (+1 more) | material: layers "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" ("Concrete Masonry Units (1)" 100., "Air" 50., "Air Infiltration Barrier" 25., "Metal Stud Layer" 100.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          8 x IFCCOLUMN | type IFCCOLUMNTYPE "100 x 190mm" | object type "M_Rectangular Column:100 x 190mm" | names: "M_Rectangular Column:100 x 190mm:293650", "M_Rectangular Column:100 x 190mm:293901", "M_Rectangular Column:100 x 190mm:293961" (+5 more) | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Gutter:Gutter:6619" | object type "Gutter:Gutter" | names: "Gutter:Gutter:294220" | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_ProductRequirements, Pset_QuantityTakeOff
          4 x IFCWINDOW | type IFCWINDOWSTYLE "1200 x 1500mm" | object type "M_Window-Casement-Double:1200 x 1500mm" | names: "M_Window-Casement-Double:1200 x 1500mm:299344", "M_Window-Casement-Double:1200 x 1500mm:299391", "M_Window-Casement-Double:1200 x 1500mm:299500" (+1 more) | material: materials ("Wood - Stained", "Glass") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon
          8 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Muntin Pattern_2x2" | object type "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2" | names: "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2:299346", "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2:299393", "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2:299491" (+5 more) | material: materials ("Clad - White", "Wood - Stained") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          8 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Muntin Pattern_2x2" | object type "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2" | names: "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2:299347", "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2:299394", "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2:299490" (+5 more) | material: materials ("Clad - White", "Wood - Stained") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "with Sill" | object type "M_Trim-Window-Exterior-Flat:with Sill" | names: "M_Trim-Window-Exterior-Flat:with Sill:299348", "M_Trim-Window-Exterior-Flat:with Sill:299395", "M_Trim-Window-Exterior-Flat:with Sill:299504" (+1 more) | material: "Clad - White" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Picture Frame" | object type "M_Trim-Window-Interior-Flat:Picture Frame" | names: "M_Trim-Window-Interior-Flat:Picture Frame:299349", "M_Trim-Window-Interior-Flat:Picture Frame:299396", "M_Trim-Window-Interior-Flat:Picture Frame:299505" (+1 more) | material: "Wood - Stained" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          4 x IFCWINDOW | type IFCWINDOWSTYLE "1200 x 1500mm" | object type "M_Window-Casement-Double:1200 x 1500mm" | names: "M_Window-Casement-Double:1200 x 1500mm:299489", "M_Window-Casement-Double:1200 x 1500mm:299494", "M_Window-Casement-Double:1200 x 1500mm:299591" (+1 more) | material: materials ("Wood - Stained", "Glass") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "with Sill" | object type "M_Trim-Window-Exterior-Flat:with Sill" | names: "M_Trim-Window-Exterior-Flat:with Sill:299492", "M_Trim-Window-Exterior-Flat:with Sill:299497", "M_Trim-Window-Exterior-Flat:with Sill:299594" (+1 more) | material: "Clad - White" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Picture Frame" | object type "M_Trim-Window-Interior-Flat:Picture Frame" | names: "M_Trim-Window-Interior-Flat:Picture Frame:299493", "M_Trim-Window-Interior-Flat:Picture Frame:299498", "M_Trim-Window-Interior-Flat:Picture Frame:299595" (+1 more) | material: "Wood - Stained" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          3 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Sofa" | object type "M_Sofa-Corbu:Sofa" | names: "M_Sofa-Corbu:Sofa:305406", "M_Sofa-Corbu:Sofa:305441", "M_Sofa-Corbu:Sofa:305472" | material: materials ("Leather - Black", "Metal - Chrome") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "0915 x 1220mm" | object type "M_Table-Dining Oval:0915 x 1220mm" | names: "M_Table-Dining Oval:0915 x 1220mm:306236" | material: "Glass - Clear, Grey" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCRAILING | object type "Railing:900mm Pipe" | names: "Railing:900mm Pipe:294046" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RailingCommon
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | object type "Level:8mm Head" | elevation 6000.
        contains 18 elements
          2 x IFCROOF | object type "Basic Roof:Tető, cserépfedés" | names: "Basic Roof:Tető, cserépfedés:289848", "Basic Roof:Tető, cserépfedés:290112" | material: layers "Basic Roof:Tető, cserépfedés" ("Default Roof" 35., "Default Roof" 25., "Default Roof" 50., "Default Roof" 75., "Default Roof" 13.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          10 x IFCBEAM | type IFCBEAMTYPE "100x400" | object type "M_Dimension Lumber:100x400" | names: "M_Dimension Lumber:100x400:292695", "M_Dimension Lumber:100x400:293066", "M_Dimension Lumber:100x400:293106" (+7 more) | material: "Softwood, Lumber" | property sets: Pset_BeamCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          6 x IFCWINDOW | type IFCWINDOWSTYLE "600 x 1200mm" | object type "M_Skylight-Top-Hung:600 x 1200mm" | names: "M_Skylight-Top-Hung:600 x 1200mm:309338", "M_Skylight-Top-Hung:600 x 1200mm:309613", "M_Skylight-Top-Hung:600 x 1200mm:309635" (+3 more) | material: materials ("Metal - Bronze, Light Brush", "Glass") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon

Types
  IFCWALLTYPE "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" | STANDARD | 9 occurrences | material: layers "Basic Wall:10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" ("Concrete Masonry Units (1)" 100., "Air" 50., "Air Infiltration Barrier" 25., "Metal Stud Layer" 100.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSLABTYPE "Floor:Vasbeton födém, úsztatott beton, parketta" | FLOOR | 1 occurrence | material: layers "Floor:Vasbeton födém, úsztatott beton, parketta" ("Default Floor" 20., "Default Floor" 50., "Default Floor" 30., "Default Floor" 200., "Default Floor" 10.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWALLTYPE "Basic Wall:Interior - 126mm Partition (2-hr)" | STANDARD | 5 occurrences | material: layers "Basic Wall:Interior - 126mm Partition (2-hr)" ("Gypsum Wall Board" 16., "Gypsum Wall Board" 16., "Metal Stud Layer" 64., "Gypsum Wall Board" 16., "Gypsum Wall Board" 16.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCDOORSTYLE "0915 x 2134mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Single-Flush:0915 x 2134mm:290838
  IFCDOORSTYLE "0915 x 2134mm" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Single-Flush:0915 x 2134mm:290867
  IFCDOORSTYLE "0762 x 2134mm" | SINGLE_SWING_RIGHT | 2 occurrences | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Single-Flush:0762 x 2134mm:290934
  IFCDOORSTYLE "0915 x 2134mm" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Single-Flush:0915 x 2134mm:291025
  IFCWINDOWSTYLE "1200 x 1500mm" | 8 occurrences | material: materials ("Wood - Stained", "Glass") | property sets: M_Window-Casement-Double:1200 x 1500mm:291112
  IFCBUILDINGELEMENTPROXYTYPE "M_Muntin Pattern_2x2" | 14 occurrences | material: materials ("Clad - White", "Wood - Stained") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_Muntin Pattern_2x2" | 14 occurrences | material: materials ("Clad - White", "Wood - Stained") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "with Sill" | 8 occurrences | material: "Clad - White" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Picture Frame" | 8 occurrences | material: "Wood - Stained" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWINDOWSTYLE "1200 x 1500mm" | 6 occurrences | material: materials ("Wood - Stained", "Glass") | property sets: M_Window-Casement-Double:1200 x 1500mm:291226
  IFCBUILDINGELEMENTPROXYTYPE "with Sill" | 6 occurrences | material: "Clad - White" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Picture Frame" | 6 occurrences | material: "Wood - Stained" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCFURNITURETYPE "1525mm Diameter" | 1 occurrence | material: materials ("Pine", "Laminate, Linen, Matte")
  IFCFURNITURETYPE "M_Chair-Breuer" | 6 occurrences | material: materials ("Textile - Bamboo Weave", "Steel, Chrome Plated")
  IFCFURNITURETYPE "1525 x 2007mm - Queen" | 2 occurrences | material: materials ("Linen, White", "Birch")
  IFCCURTAINWALLTYPE "Curtain Wall:Storefront" | 1 occurrence | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "8,5" | 1 occurrence | material: "Pine" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Largetooth Aspen - 7.6 Meters" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Lombardy Poplar - 12.2 Meters" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Red Ash - 7.6 Meters" | 3 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "8,5" | 1 occurrence | material: "Pine" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "535 x 910 x 810mm" | 1 occurrence | material: "Steel, Paint Finish, Ivory, Glossy" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCSLABTYPE "Floor:Vasbeton födém, úsztatott beton, parketta" | FLOOR | 1 occurrence | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOLUMNTYPE "100 x 190mm" | COLUMN | 8 occurrences | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCPIPESEGMENTTYPE "Gutter:Gutter:6619" | element type "Gutter:Gutter:6619" | GUTTER | 1 occurrence
  IFCFURNITURETYPE "Sofa" | 3 occurrences | material: materials ("Leather - Black", "Metal - Chrome")
  IFCFURNITURETYPE "0915 x 1220mm" | 1 occurrence | material: "Glass - Clear, Grey"
  IFCBEAMTYPE "100x400" | BEAM | 10 occurrences | property sets: Pset_BeamCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
  IFCWINDOWSTYLE "600 x 1200mm" | 6 occurrences | material: materials ("Metal - Bronze, Light Brush", "Glass") | property sets: M_Skylight-Top-Hung:600 x 1200mm:309338

Property sets
  Pset_ProductRequirements | properties | on 63 objects (63 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
  Pset_ProductRequirements | properties | on 58 objects (58 IFCBUILDINGELEMENTPROXY) | on 8 type objects
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 25 objects (25 IFCPLATE)
    Category = "Curtain Panels" (IFCLABEL)
  Pset_ProductRequirements | properties | on 20 objects (20 IFCWINDOW)
    Category = "Windows" (IFCLABEL)
  Pset_ProductRequirements | properties | on 15 objects (9 IFCWALLSTANDARDCASE, 5 IFCWALL, 1 IFCCURTAINWALL) | on 3 type objects
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 13 objects (13 IFCFURNISHINGELEMENT)
    Category = "Furniture" (IFCLABEL)
  Pset_ProductRequirements | properties | on 10 objects (10 IFCBEAM) | on 1 type object
    Category = "Structural Framing" (IFCLABEL)
  Pset_ProductRequirements | properties | on 8 objects (8 IFCCOLUMN) | on 1 type object
    Category = "Columns" (IFCLABEL)
  Pset_ProductRequirements: 19 more contents on 38 objects not shown
  Pset_ElementShading | properties | on 20 objects (9 IFCWALLSTANDARDCASE, 5 IFCWALL, 2 IFCOPENINGELEMENT, 2 IFCROOF) | on 4 type objects
    Roughness = 914.4 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_QuantityTakeOff | properties | on 63 objects (63 IFCMEMBER)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 28 objects (28 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "M_Muntin Pattern_2x2" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 25 objects (25 IFCPLATE)
    Reference = "Glazed" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "with Sill" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "Picture Frame" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 14 objects (14 IFCWINDOW)
    Reference = "1200 x 1500mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 10 objects (10 IFCBEAM) | on 1 type object
    Reference = "100x400" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 9 objects (5 IFCWALL, 4 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 25 more contents on 65 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 9 objects (5 IFCWALL, 4 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 5 objects (5 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Interior - 126mm Partition (2-hr)" (IFCLABEL)
  Pset_WallCommon | properties | on 5 objects (4 IFCWALLSTANDARDCASE, 1 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" (IFCIDENTIFIER)
    ThermalTransmittance = 0.153998025666338 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 5 objects (5 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Interior - 126mm Partition (2-hr)" (IFCIDENTIFIER)
    ThermalTransmittance = 0.376157407407407 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" (IFCIDENTIFIER)
    ThermalTransmittance = 0.153998025666338 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" (IFCIDENTIFIER)
    ThermalTransmittance = 0.153998025666338 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "10cm beton blokk, hőszigetelés, átszellőztetett téglaburkolat" (IFCIDENTIFIER)
    ThermalTransmittance = 0.153998025666338 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Interior - 126mm Partition (2-hr)" (IFCIDENTIFIER)
    ThermalTransmittance = 0.376157407407407 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB) | on 2 type objects
    Reference = "Vasbeton födém, úsztatott beton, parketta" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Vasbeton födém, úsztatott beton, parketta" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Vasbeton födém, úsztatott beton, parketta" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Vasbeton födém, úsztatott beton, parketta" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 2 objects (2 IFCOPENINGELEMENT)
    Reference = "Vasbeton födém, úsztatott beton, parketta" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 58.0053125 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Tető, cserépfedés" (IFCIDENTIFIER)
    TotalArea = 83.0357034270203 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 58.0053125 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Tető, cserépfedés" (IFCIDENTIFIER)
    TotalArea = 80.3118269334146 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_DoorCommon | properties | on 3 objects (3 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0915 x 2134mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0762 x 2134mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 14 objects (14 IFCWINDOW)
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "1200 x 1500mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 6 objects (6 IFCWINDOW)
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "600 x 1200mm" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 28 objects (28 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "M_Muntin Pattern_2x2" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "with Sill" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "Picture Frame" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Red Ash - 7.6 Meters" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "8,5" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Largetooth Aspen - 7.6 Meters" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Lombardy Poplar - 12.2 Meters" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "535 x 910 x 810mm" (IFCIDENTIFIER)
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 23. (IFCCOUNTMEASURE)
    NumberOfTreads = 22. (IFCCOUNTMEASURE)
    Reference = "Monolithic Stair" (IFCIDENTIFIER)
    RiserHeight = 145. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 275. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 23. (IFCCOUNTMEASURE)
    NumberOfTreads = 22. (IFCCOUNTMEASURE)
    Reference = "25mm Nosing" (IFCIDENTIFIER)
    RiserHeight = 145. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 275. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 275. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WaistThickness = 1000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 500. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 10 objects (10 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "100x400" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 6200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "100x400" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfBeam | properties | on 10 objects (10 IFCBEAM) | on 1 type object
    Reference = "100x400" (IFCLABEL)
  Pset_ColumnCommon | properties | on 8 objects (8 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "100 x 190mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "100 x 190mm" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfColumn | properties | on 8 objects (8 IFCCOLUMN) | on 1 type object
    Reference = "100 x 190mm" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 2 objects (2 IFCFLOWTERMINAL)
    Reference = "760 x 535mm" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWSEGMENT)
    Reference = "Gutter" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "M_Toilet-Domestic-3D" (IFCIDENTIFIER)
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 20950. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 20950. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_RampFlightCommon | properties | on 3 objects (3 IFCRAMPFLIGHT)
    Reference = "Ramp 1" (IFCIDENTIFIER)
  Pset_RampCommon | properties | on 3 objects (3 IFCRAMP)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Ramp 1" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Storefront" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Storefront" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 25 objects (25 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Glazed" (IFCIDENTIFIER)
    ThermalTransmittance = 6.7069 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_MemberCommon | properties | on 12 objects (12 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 899.9999998476 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 9 objects (9 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 800. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 9 objects (9 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 1600. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 8 objects (8 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 150. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 8 objects (8 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 75. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 8 objects (8 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 500.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 4 objects (4 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 875.0000001524 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 125. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon: 2 more contents on 3 objects not shown
  Pset_RailingCommon | properties | on 1 object (1 IFCRAILING)
    Height = 900. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "900mm Pipe" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "T.O. Slab" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "T.O. Fnd. Wall" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 0" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 2" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 5 (IFCINTEGER)
  M_Single-Flush:0915 x 2134mm:290838 | predefined | on 2 type objects
  M_Single-Flush:0915 x 2134mm:290867 | predefined | on 2 type objects
  M_Single-Flush:0762 x 2134mm:290934 | predefined | on 2 type objects
  M_Single-Flush:0915 x 2134mm:291025 | predefined | on 2 type objects
  M_Window-Casement-Double:1200 x 1500mm:291112 | predefined | on 1 type object
  M_Window-Casement-Double:1200 x 1500mm:291226 | predefined | on 1 type object
  M_Skylight-Top-Hung:600 x 1200mm:309338 | predefined | on 1 type object

Other addresses and roles
  2 x postal address: "Enter address here", "Boston", "MA"