IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "0001"
Time stamp: "2020-02-17T13:55:59"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190327_2315(x64) - Exporter 20.0.0.377 - Alternate UI 20.0.0.377"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "User_05" of Organization (no name given)
  Owner history of Person "User_05" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1581943659 (2020-02-17T12:47:39Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "01 Level" | long name "01 Level" | object type "Level:8mm Head" | elevation 4000.
        contains 6 elements
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Rectangular Duct:Air" | object type "Rectangular Duct:Air" | names: "Rectangular Duct:Air:549554", "Rectangular Duct:Air:611850", "Rectangular Duct:Air:612560" (+1 more) | property sets: Constraints, Dimensions, Insulation, Lining, Mechanical, Mechanical - Flow
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | object type "magirect_elbow1_001:Supplay Air_Elbow_Rect" | names: "magirect_elbow1_001:Supplay Air_Elbow_Rect:616751", "magirect_elbow1_001:Supplay Air_Elbow_Rect:616762" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
      IFCBUILDINGSTOREY "02 Level" | long name "02 Level" | object type "Level:8mm Head" | elevation 8000.
        contains 1 element
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | object type "magirect_tbranch1_001:Supplay Air_Tbranch_Rect" | names: "magirect_tbranch1_001:Supplay Air_Tbranch_Rect:604962" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
      IFCBUILDINGSTOREY "03 Level" | long name "03 Level" | object type "Level:8mm Head" | elevation 12000.
        contains 20 elements
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Round Duct:Air" | object type "Round Duct:Air" | names: "Round Duct:Air:606103", "Round Duct:Air:606107", "Round Duct:Air:610366" (+1 more) | property sets: Constraints, Dimensions, Insulation, Lining, Mechanical, Mechanical - Flow
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Rectangular Duct:Air" | object type "Rectangular Duct:Air" | names: "Rectangular Duct:Air:606105", "Rectangular Duct:Air:606111", "Rectangular Duct:Air:610368" (+1 more) | property sets: Constraints, Dimensions, Insulation, Lining, Mechanical, Mechanical - Flow
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | object type "magirect_tbranch1_001:Supplay Air_Tbranch_Rect" | names: "magirect_tbranch1_001:Supplay Air_Tbranch_Rect:606106" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | object type "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ" | names: "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ:606109", "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ:606117" | material: "Material_Duct" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WK25 250 250-1" | object type "WK25-0001:WK25 250 250-1" | names: "WK25-0001:WK25 250 250-1:606110" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | object type "magirect_tbranch1_001:Supplay Air_Tbranch_Rect" | names: "magirect_tbranch1_001:Supplay Air_Tbranch_Rect:606124" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_LRD" | object type "Lindab LDR:Supplay Air_LRD" | names: "Lindab LDR:Supplay Air_LRD:606125" | material: "DF_Material1" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | object type "magirect_tbranch1_001:Supplay Air_Tbranch_Rect" | names: "magirect_tbranch1_001:Supplay Air_Tbranch_Rect:610369" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | object type "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ" | names: "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ:610372", "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ:610380" | material: "Material_Duct" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WK25 250 250-1" | object type "WK25-0001:WK25 250 250-1" | names: "WK25-0001:WK25 250 250-1:610373" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | object type "magirect_tbranch1_001:Supplay Air_Tbranch_Rect" | names: "magirect_tbranch1_001:Supplay Air_Tbranch_Rect:610387" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_LRD" | object type "Lindab LDR:Supplay Air_LRD" | names: "Lindab LDR:Supplay Air_LRD:610388" | material: "DF_Material1" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
      IFCBUILDINGSTOREY "04 Roof" | long name "04 Roof" | object type "Level:8mm Head" | elevation 16000.
        contains 28 elements
          15 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Rectangular Duct:Air" | object type "Rectangular Duct:Air" | names: "Rectangular Duct:Air:615774", "Rectangular Duct:Air:616264", "Rectangular Duct:Air:616639" (+12 more) | property sets: Constraints, Dimensions, Insulation, Lining, Mechanical, Mechanical - Flow
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Standard" | object type "M_Rectangular Offset - Plain - Flanged:Standard" | names: "M_Rectangular Offset - Plain - Flanged:Standard:618180", "M_Rectangular Offset - Plain - Flanged:Standard:618548" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | object type "magirect_elbow1_001:Supplay Air_Elbow_Rect" | names: "magirect_elbow1_001:Supplay Air_Elbow_Rect:618376", "magirect_elbow1_001:Supplay Air_Elbow_Rect:618635", "magirect_elbow1_001:Supplay Air_Elbow_Rect:618664" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | object type "magirect_tbranch1_001:Supplay Air_Tbranch_Rect" | names: "magirect_tbranch1_001:Supplay Air_Tbranch_Rect:618743" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Standard" | object type "M_Rectangular Offset - Plain - Flanged:Standard" | names: "M_Rectangular Offset - Plain - Flanged:Standard:624393" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | object type "magirect_elbow1_001:Supplay Air_Elbow_Rect" | names: "magirect_elbow1_001:Supplay Air_Elbow_Rect:629611", "magirect_elbow1_001:Supplay Air_Elbow_Rect:630258" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | object type "magirect_elbow1_001:Supplay Air_Elbow_Rect" | names: "magirect_elbow1_001:Supplay Air_Elbow_Rect:630256" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WK25 700 250-1" | object type "WK25-0001:WK25 700 250-1" | names: "WK25-0001:WK25 700 250-1:630453" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_LRD" | object type "Lindab LDR:Supplay Air_LRD" | names: "Lindab LDR:Supplay Air_LRD:630737" | material: "DF_Material1" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics

Types
  IFCDUCTSEGMENTTYPE "Rectangular Duct:Air" | 23 occurrences | property sets: Construction, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | 2 occurrences | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | 2 occurrences | property sets: Constraints, Identity Data, Other
  IFCDUCTSEGMENTTYPE "Round Duct:Air" | 4 occurrences | property sets: Construction, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | 1 occurrence | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | 2 occurrences | material: "Material_Duct" | property sets: Constraints, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "WK25 250 250-1" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | 1 occurrence | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_LRD" | 1 occurrence | material: "DF_Material1" | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | 1 occurrence | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | 2 occurrences | material: "Material_Duct" | property sets: Constraints, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "WK25 250 250-1" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCDUCTFITTINGTYPE "Supplay Air_LRD" | 1 occurrence | material: "DF_Material1" | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Standard" | 2 occurrences | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | 4 occurrences | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | 1 occurrence | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Standard" | 1 occurrence | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | 2 occurrences | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | 1 occurrence | property sets: Constraints, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "WK25 700 250-1" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCDUCTFITTINGTYPE "Supplay Air_LRD" | 1 occurrence | material: "DF_Material1" | property sets: Constraints, Identity Data, Other

Property sets
  Other | properties | on 46 objects (46 IFCFLOWSEGMENT)
    Category = "Ducts" (IFCLABEL)
    Family = "Rectangular Duct: Air" (IFCLABEL)
    Family and Type = "Rectangular Duct: Air" (IFCLABEL)
    Type = "Rectangular Duct: Air" (IFCLABEL)
    Type Id = "Rectangular Duct: Air" (IFCLABEL)
  Other | properties | on 9 objects (9 IFCFLOWFITTING)
    Category = "Duct Fittings" (IFCLABEL)
    Family = "magirect_elbow1_001: Supplay Air_Elbow_Rect" (IFCLABEL)
    Family and Type = "magirect_elbow1_001: Supplay Air_Elbow_Rect" (IFCLABEL)
    Type = "magirect_elbow1_001: Supplay Air_Elbow_Rect" (IFCLABEL)
    Type Id = "magirect_elbow1_001: Supplay Air_Elbow_Rect" (IFCLABEL)
  Other | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Category = "Ducts" (IFCLABEL)
    Family = "Round Duct: Air" (IFCLABEL)
    Family and Type = "Round Duct: Air" (IFCLABEL)
    Type = "Round Duct: Air" (IFCLABEL)
    Type Id = "Round Duct: Air" (IFCLABEL)
  Other | properties | on 6 objects (6 IFCFLOWFITTING)
    Category = "Duct Fittings" (IFCLABEL)
    Family = "magirect_tbranch1_001: Supplay Air_Tbranch_Rect" (IFCLABEL)
    Family and Type = "magirect_tbranch1_001: Supplay Air_Tbranch_Rect" (IFCLABEL)
    Type = "magirect_tbranch1_001: Supplay Air_Tbranch_Rect" (IFCLABEL)
    Type Id = "magirect_tbranch1_001: Supplay Air_Tbranch_Rect" (IFCLABEL)
  Other | properties | on 4 objects (4 IFCSYSTEM)
    Category = "Duct Systems" (IFCLABEL)
    Family = "Duct System: D3060.10.-BEFÚVÁS" (IFCLABEL)
    Family and Type = "Duct System: D3060.10.-BEFÚVÁS" (IFCLABEL)
    Type = "Duct System: D3060.10.-BEFÚVÁS" (IFCLABEL)
    Type Id = "Duct System: D3060.10.-BEFÚVÁS" (IFCLABEL)
  Other | properties | on 4 objects (4 IFCFLOWFITTING)
    Category = "Duct Fittings" (IFCLABEL)
    Family = "magicirc_multi_shape_trans_001: Supplay Air_Multi shape transition_Circ" (IFCLABEL)
    Family and Type = "magicirc_multi_shape_trans_001: Supplay Air_Multi shape transition_Circ" (IFCLABEL)
    Type = "magicirc_multi_shape_trans_001: Supplay Air_Multi shape transition_Circ" (IFCLABEL)
    Type Id = "magicirc_multi_shape_trans_001: Supplay Air_Multi shape transition_Circ" (IFCLABEL)
    Visibility_Ins = FALSE (IFCBOOLEAN)
    Visibility_Lining = FALSE (IFCBOOLEAN)
  Other | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 3 objects (3 IFCFLOWFITTING)
    Category = "Duct Fittings" (IFCLABEL)
    Family = "Lindab LDR: Supplay Air_LRD" (IFCLABEL)
    Family and Type = "Lindab LDR: Supplay Air_LRD" (IFCLABEL)
    Type = "Lindab LDR: Supplay Air_LRD" (IFCLABEL)
    Type Id = "Lindab LDR: Supplay Air_LRD" (IFCLABEL)
  Other: 13 more contents on 8 objects not shown
  Mechanical - Flow | properties | on 54 objects (54 IFCFLOWSEGMENT)
    Additional Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Friction = 0. (IFCREAL) [derived "Friction Loss"]
    Pressure Drop = 0. (IFCPRESSUREMEASURE) [PASCAL]
    Reynolds number = 0. (IFCREAL)
    Velocity = 0. (IFCLINEARVELOCITYMEASURE) [derived]
    Velocity Pressure = 0. (IFCPRESSUREMEASURE) [PASCAL]
  Mechanical - Flow | properties | on 8 objects (6 IFCFLOWFITTING, 2 IFCBUILDINGELEMENTPROXY)
    Pressure Drop = 0. (IFCPRESSUREMEASURE) [PASCAL]
  Mechanical - Flow | properties | on 4 objects (4 IFCSYSTEM)
    Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "21" (IFCTEXT)
    Productdata = "© Progman Oy, all rights reserved" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "27" (IFCTEXT)
    Productdata = "© Progman Oy, all rights reserved" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "34" (IFCTEXT)
    Productdata = "© Progman Oy, all rights reserved" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "01 Level" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "02 Level" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "03 Level" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "04 Roof" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data: 9 more contents on 0 objects not shown
  Constraints | properties | on 16 objects (16 IFCFLOWSEGMENT)
    Bottom Elevation = 3385. (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 3510. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 3510. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 03 Level" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 3510. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 3635. (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 12 objects (10 IFCFLOWFITTING, 2 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 3510. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: 03 Level" (IFCLABEL)
  Constraints | properties | on 10 objects (10 IFCFLOWSEGMENT)
    Bottom Elevation = 1410.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 1535.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 1535.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 04 Roof" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 1535.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 1660.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Bottom Elevation = 1110.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 1235.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 1235.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 04 Roof" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 1235.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 1360.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Bottom Elevation = 1110.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 1235.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 1235.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 04 Roof" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 1235.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 1360.95052634351 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Bottom Elevation = 4605.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 4780.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 4780.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 04 Roof" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 4780.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 4955.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 3 objects (3 IFCFLOWFITTING)
    Elevation from Level = 1235.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: 04 Roof" (IFCLABEL)
  Constraints | properties | on 3 objects (3 IFCFLOWFITTING)
    Elevation from Level = 1535.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: 04 Roof" (IFCLABEL)
  Constraints: 21 more contents on 30 objects not shown
  Dimensions | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Height = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 1350.95052634352 (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "350 mmx250 mm" (IFCTEXT)
    Width = 350. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Diameter = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 1675.67988537007 (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "250 mmø" (IFCTEXT)
  Dimensions | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Height = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 334.049748133151 (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "250 mmx250 mm" (IFCTEXT)
    Width = 250. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Diameter = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 1633.4100106998 (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "250 mmø" (IFCTEXT)
  Dimensions | properties | on 4 objects (4 IFCFLOWFITTING)
    Diameter = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    H0 = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    H0/2 = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    Insulation H0 = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Insulation Radius = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    Insulation W0 = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    L = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    Lining H0 = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Lining Radius = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    Lining W0 = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    OffsetHeight = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    OffsetHeightTemp = 0.0341754155730534 (IFCREAL)
    OffsetHeightfromBase = 3048. (IFCLENGTHMEASURE) [MILLI METRE]
    OffsetWidth = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    OffsetWidthTemp = -0.0341754155730534 (IFCREAL)
    OffsetWidthfromBase = 3048. (IFCLENGTHMEASURE) [MILLI METRE]
    Radius = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "250 mmx250 mm-250 mmø" (IFCTEXT)
    Volume = 0.00145072821010284 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    W0 = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    W0/2 = 125. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Height = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 3386.61256268045 (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "250 mmx250 mm" (IFCTEXT)
    Width = 250. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 4 objects (4 IFCFLOWFITTING)
    Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Angle_list = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    B_Lining = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    Bout = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    Bout_Ins = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    H_Lining = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Hout = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Hout_Ins = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    L = 275. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "350 mmx250 mm-350 mmx250 mm" (IFCTEXT)
    ThroatR = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Visibility_Ins = FALSE (IFCBOOLEAN)
    Visibility_Lining = FALSE (IFCBOOLEAN)
    Volume = 0.0377971374415954 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    rc = 275. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions: 31 more contents on 54 objects not shown
  Insulation | properties | on 24 objects (24 IFCFLOWSEGMENT)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "350 mmx250 mm" (IFCTEXT)
  Insulation | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "250 mmø" (IFCTEXT)
  Insulation | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "250 mmx250 mm" (IFCTEXT)
  Insulation | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "700 mmx350 mm" (IFCTEXT)
  Insulation | properties | on 6 objects (6 IFCFLOWSEGMENT)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "700 mmx250 mm" (IFCTEXT)
  Insulation | properties | on 4 objects (4 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "250 mmx250 mm-250 mmø" (IFCTEXT)
  Insulation | properties | on 4 objects (4 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "250 mmx350 mm-250 mmx350 mm" (IFCTEXT)
  Insulation | properties | on 4 objects (4 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "350 mmx250 mm-350 mmx250 mm" (IFCTEXT)
  Insulation: 10 more contents on 16 objects not shown
  Lining | properties | on 24 objects (24 IFCFLOWSEGMENT)
    Free Size = "350 mmx250 mm" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Free Size = "250 mmø" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Free Size = "250 mmx250 mm" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Free Size = "700 mmx350 mm" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining | properties | on 6 objects (6 IFCFLOWSEGMENT)
    Free Size = "700 mmx250 mm" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining | properties | on 4 objects (4 IFCFLOWFITTING)
    Free Size = "250 mmx250 mm-250 mmø" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining | properties | on 4 objects (4 IFCFLOWFITTING)
    Free Size = "250 mmx350 mm-250 mmx350 mm" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining | properties | on 4 objects (4 IFCFLOWFITTING)
    Free Size = "350 mmx250 mm-350 mmx250 mm" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining: 10 more contents on 16 objects not shown
  Mechanical | properties | on 6 objects (3 IFCBUILDINGELEMENTPROXY, 3 IFCFLOWFITTING)
    Loss Method = "8baf7d75-8b9b-46d0-b8ce-3ad1c19e6b19" (IFCTEXT)
    System Abbreviation = "BL" (IFCTEXT)
    System Classification = "Supply Air" (IFCTEXT)
    System Name = "Mechanical D3060.10.-BEFÚVÁS 7" (IFCTEXT)
    System Type = "Duct System: D3060.10.-BEFÚVÁS" (IFCLABEL)
  Mechanical | properties | on 4 objects (4 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Method = "8baf7d75-8b9b-46d0-b8ce-3ad1c19e6b19" (IFCTEXT)
    MC_B = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    MC_H = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    MC_R = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    System Abbreviation = "BL" (IFCTEXT)
    System Classification = "Supply Air" (IFCTEXT)
    System Name = "Mechanical D3060.10.-BEFÚVÁS 7" (IFCTEXT)
    System Type = "Duct System: D3060.10.-BEFÚVÁS" (IFCLABEL)
  Mechanical | properties | on 4 objects (4 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Method = "8baf7d75-8b9b-46d0-b8ce-3ad1c19e6b19" (IFCTEXT)
    MC_B = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    MC_H = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    System Abbreviation = "BL" (IFCTEXT)
    System Classification = "Supply Air" (IFCTEXT)
    System Name = "Mechanical D3060.10.-BEFÚVÁS 7" (IFCTEXT)
    System Type = "Duct System: D3060.10.-BEFÚVÁS" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 1.62114063161222 (IFCAREAMEASURE) [SQUARE_METRE]
    Equivalent Diameter = 322.225994577572 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydraulic Diameter = 291.666666666667 (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Coefficient = 0. (IFCREAL)
    Section = 20 (IFCINTEGER)
    Size Lock = FALSE (IFCBOOLEAN)
    System Abbreviation = "BL" (IFCTEXT)
    System Classification = "Supply Air" (IFCTEXT)
    System Name = "Mechanical D3060.10.-BEFÚVÁS 7" (IFCTEXT)
    System Type = "Duct System: D3060.10.-BEFÚVÁS" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 1.3160759044117 (IFCAREAMEASURE) [SQUARE_METRE]
    Equivalent Diameter = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydraulic Diameter = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Coefficient = 0. (IFCREAL)
    Section = 17 (IFCINTEGER)
    Size Lock = FALSE (IFCBOOLEAN)
    System Abbreviation = "BL" (IFCTEXT)
    System Classification = "Supply Air" (IFCTEXT)
    System Name = "Mechanical D3060.10.-BEFÚVÁS 7" (IFCTEXT)
    System Type = "Duct System: D3060.10.-BEFÚVÁS" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 0.334049748133151 (IFCAREAMEASURE) [SQUARE_METRE]
    Equivalent Diameter = 273.291334957457 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydraulic Diameter = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Coefficient = 0. (IFCREAL)
    Section = 12 (IFCINTEGER)
    Size Lock = FALSE (IFCBOOLEAN)
    System Abbreviation = "BL" (IFCTEXT)
    System Classification = "Supply Air" (IFCTEXT)
    System Name = "Mechanical D3060.10.-BEFÚVÁS 7" (IFCTEXT)
    System Type = "Duct System: D3060.10.-BEFÚVÁS" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Method = "8baf7d75-8b9b-46d0-b8ce-3ad1c19e6b19" (IFCTEXT)
    MC_B1 = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    MC_B3 = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    MC_H1 = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    System Abbreviation = "BL" (IFCTEXT)
    System Classification = "Supply Air" (IFCTEXT)
    System Name = "Mechanical D3060.10.-BEFÚVÁS 7" (IFCTEXT)
    System Type = "Duct System: D3060.10.-BEFÚVÁS" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 1.28287722247863 (IFCAREAMEASURE) [SQUARE_METRE]
    Equivalent Diameter = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydraulic Diameter = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Coefficient = 0. (IFCREAL)
    Section = 19 (IFCINTEGER)
    Size Lock = FALSE (IFCBOOLEAN)
    System Abbreviation = "BL" (IFCTEXT)
    System Classification = "Supply Air" (IFCTEXT)
    System Name = "Mechanical D3060.10.-BEFÚVÁS 7" (IFCTEXT)
    System Type = "Duct System: D3060.10.-BEFÚVÁS" (IFCLABEL)
  Mechanical: 35 more contents on 62 objects not shown
  Phasing | properties | on 82 objects (54 IFCFLOWSEGMENT, 25 IFCFLOWFITTING, 3 IFCBUILDINGELEMENTPROXY)
    Phase Created = "Phase 1" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 27 objects (27 IFCFLOWSEGMENT)
    Reference = "Air" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 9 objects (9 IFCFLOWFITTING)
    Reference = "Supplay Air_Elbow_Rect" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 6 objects (6 IFCFLOWFITTING)
    Reference = "Supplay Air_Tbranch_Rect" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 4 objects (4 IFCFLOWFITTING)
    Reference = "Supplay Air_Multi shape transition_Circ" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 3 objects (3 IFCFLOWFITTING)
    Reference = "Supplay Air_LRD" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 3 objects (3 IFCFLOWFITTING)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 27 objects (27 IFCFLOWSEGMENT)
    Roughness = 0.150000005960465 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 1350.95052634352 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 1675.67988537007 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 334.049748133151 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 1633.4100106998 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 3386.61256268045 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 3900. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 3700. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 536.322509939066 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment: 14 more contents on 14 objects not shown
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 1350.95052634352 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 1675.67988537007 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 334.049748133151 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 1633.4100106998 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 3386.61256268045 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 3900. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 3700. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 536.322509939066 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment: 14 more contents on 14 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 23 objects (23 IFCFLOWSEGMENT)
    Manufacturer = "Generic" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Manufacturer (no value)
  Pset_ManufacturerTypeInformation | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Manufacturer = "Lindab" (IFCLABEL)
  Pset_ProductRequirements | properties | on 27 objects (27 IFCFLOWSEGMENT)
    Category = "Ducts" (IFCLABEL)
  Pset_ProductRequirements | properties | on 25 objects (25 IFCFLOWFITTING)
    Category = "Duct Fittings" (IFCLABEL)
  Pset_ProductRequirements | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Category = "Duct Accessories" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "01 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "02 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "03 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "04 Roof" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 27 objects (27 IFCFLOWSEGMENT)
    Reference = "Air" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 9 objects (9 IFCFLOWFITTING)
    Reference = "Supplay Air_Elbow_Rect" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 6 objects (6 IFCFLOWFITTING)
    Reference = "Supplay Air_Tbranch_Rect" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCFLOWFITTING)
    Reference = "Supplay Air_Multi shape transition_Circ" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 3 objects (3 IFCFLOWFITTING)
    Reference = "Supplay Air_LRD" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 3 objects (3 IFCFLOWFITTING)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "WK25 250 250-1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "WK25 700 250-1" (IFCIDENTIFIER)
  Graphics | properties | on 16 objects (13 IFCFLOWFITTING, 3 IFCBUILDINGELEMENTPROXY)
    Use Annotation Scale = FALSE (IFCBOOLEAN)
  Graphics | properties | on 9 objects (9 IFCFLOWFITTING)
    Segmented = FALSE (IFCBOOLEAN)
    SubTp = 2 (IFCINTEGER)
    Use Annotation Scale = FALSE (IFCBOOLEAN)
  Graphics | properties | on 3 objects (3 IFCFLOWFITTING)
    Use Annotation Scale = FALSE (IFCBOOLEAN)
    hasPyramid = TRUE (IFCBOOLEAN)
  Materials and Finishes | properties | on 4 objects (4 IFCFLOWFITTING)
    Material_Duct = "Material_Duct" (IFCLABEL)
    Material_Ins = "Material_Ins" (IFCLABEL)
    Material_Lining = "Material_Lining" (IFCLABEL)
  Materials and Finishes | properties | on 3 objects (3 IFCFLOWFITTING)
    DF_Material1 = "DF_Material1" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "WK25 250 250-1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "WK25 700 250-1" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "01 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "02 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "03 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "04 Roof" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 4 (IFCINTEGER)
  Constraints(Type) | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Other(Type) | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Construction | properties | on 2 type objects
    Roughness = 0.150000005960465 (IFCLENGTHMEASURE) [MILLI METRE]

Other addresses and roles
  2 x postal address: "Enter address here", "Boston", "MA"