IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "0001"
Time stamp: "2020-02-17T13:52:38"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190327_2315(x64) - Exporter 20.0.0.377 - Alternate UI 20.0.0.377"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "User_05" of Organization (no name given)
  Owner history of Person "User_05" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1581943659 (2020-02-17T12:47:39Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "01 Level" | long name "01 Level" | object type "Level:8mm Head" | elevation 4000.
        contains 5 elements
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Rectangular Duct:Air" | object type "Rectangular Duct:Air" | names: "Rectangular Duct:Air:549157", "Rectangular Duct:Air:611849", "Rectangular Duct:Air:614214" (+1 more) | property sets: Constraints, Dimensions, Insulation, Lining, Mechanical, Mechanical - Flow
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | object type "magirect_elbow1_001:Supplay Air_Elbow_Rect" | names: "magirect_elbow1_001:Supplay Air_Elbow_Rect:620254" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
      IFCBUILDINGSTOREY "03 Level" | long name "03 Level" | object type "Level:8mm Head" | elevation 12000.
        contains 46 elements
          18 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Round Duct:Air" | object type "Round Duct:Air" | names: "Round Duct:Air:606063", "Round Duct:Air:606065", "Round Duct:Air:606067" (+15 more) | property sets: Constraints, Dimensions, Insulation, Lining, Mechanical, Mechanical - Flow
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Elbow short_Circ" | object type "magicirc_elbow_short_001:Supplay Air_Elbow short_Circ" | names: "magicirc_elbow_short_001:Supplay Air_Elbow short_Circ:606069", "magicirc_elbow_short_001:Supplay Air_Elbow short_Circ:606090" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WK25 200 200-1" | object type "WK25-0001:WK25 200 200-1" | names: "WK25-0001:WK25 200 200-1:606078" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Rectangular Duct:Air" | object type "Rectangular Duct:Air" | names: "Rectangular Duct:Air:606079", "Rectangular Duct:Air:606095", "Rectangular Duct:Air:610342" (+1 more) | property sets: Constraints, Dimensions, Insulation, Lining, Mechanical, Mechanical - Flow
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Elbow short_Circ" | object type "magicirc_elbow_short_001:Supplay Air_Elbow short_Circ" | names: "magicirc_elbow_short_001:Supplay Air_Elbow short_Circ:606080", "magicirc_elbow_short_001:Supplay Air_Elbow short_Circ:606082", "magicirc_elbow_short_001:Supplay Air_Elbow short_Circ:606098" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Tee centric 90_Circ" | object type "magicirc_tee_centric_90_001:Supplay Air_Tee centric 90_Circ" | names: "magicirc_tee_centric_90_001:Supplay Air_Tee centric 90_Circ:606086" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Reduction_Circ" | object type "magicirc_reduction_001:Supplay Air_Reduction_Circ" | names: "magicirc_reduction_001:Supplay Air_Reduction_Circ:606092" | material: "Material_Duct" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | object type "magirect_tbranch1_001:Supplay Air_Tbranch_Rect" | names: "magirect_tbranch1_001:Supplay Air_Tbranch_Rect:606094" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | object type "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ" | names: "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ:606096" | material: "Material_Duct" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | object type "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ" | names: "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ:606100" | material: "Material_Duct" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | object type "magirect_tbranch1_001:Supplay Air_Tbranch_Rect" | names: "magirect_tbranch1_001:Supplay Air_Tbranch_Rect:606123" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Elbow short_Circ" | object type "magicirc_elbow_short_001:Supplay Air_Elbow short_Circ" | names: "magicirc_elbow_short_001:Supplay Air_Elbow short_Circ:610332", "magicirc_elbow_short_001:Supplay Air_Elbow short_Circ:610353" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WK25 200 200-1" | object type "WK25-0001:WK25 200 200-1" | names: "WK25-0001:WK25 200 200-1:610341" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Elbow short_Circ" | object type "magicirc_elbow_short_001:Supplay Air_Elbow short_Circ" | names: "magicirc_elbow_short_001:Supplay Air_Elbow short_Circ:610343", "magicirc_elbow_short_001:Supplay Air_Elbow short_Circ:610345", "magicirc_elbow_short_001:Supplay Air_Elbow short_Circ:610361" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Tee centric 90_Circ" | object type "magicirc_tee_centric_90_001:Supplay Air_Tee centric 90_Circ" | names: "magicirc_tee_centric_90_001:Supplay Air_Tee centric 90_Circ:610349" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Reduction_Circ" | object type "magicirc_reduction_001:Supplay Air_Reduction_Circ" | names: "magicirc_reduction_001:Supplay Air_Reduction_Circ:610355" | material: "Material_Duct" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | object type "magirect_tbranch1_001:Supplay Air_Tbranch_Rect" | names: "magirect_tbranch1_001:Supplay Air_Tbranch_Rect:610357" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | object type "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ" | names: "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ:610359" | material: "Material_Duct" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | object type "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ" | names: "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ:610363" | material: "Material_Duct" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | object type "magirect_tbranch1_001:Supplay Air_Tbranch_Rect" | names: "magirect_tbranch1_001:Supplay Air_Tbranch_Rect:610386" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
      IFCBUILDINGSTOREY "04 Roof" | long name "04 Roof" | object type "Level:8mm Head" | elevation 16000.
        contains 27 elements
          12 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Rectangular Duct:Air" | object type "Rectangular Duct:Air" | names: "Rectangular Duct:Air:615809", "Rectangular Duct:Air:616238", "Rectangular Duct:Air:619926" (+9 more) | property sets: Constraints, Dimensions, Insulation, Lining, Mechanical, Mechanical - Flow
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | object type "magirect_elbow1_001:Supplay Air_Elbow_Rect" | names: "magirect_elbow1_001:Supplay Air_Elbow_Rect:616281", "magirect_elbow1_001:Supplay Air_Elbow_Rect:619959", "magirect_elbow1_001:Supplay Air_Elbow_Rect:620252" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | object type "magirect_elbow1_001:Supplay Air_Elbow_Rect" | names: "magirect_elbow1_001:Supplay Air_Elbow_Rect:620246" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "AXC-800-9-4" | object type "AXC:AXC-800-9-4" | names: "AXC:AXC-800-9-4:621663" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | object type "magirect_elbow1_001:Supplay Air_Elbow_Rect" | names: "magirect_elbow1_001:Supplay Air_Elbow_Rect:622086", "magirect_elbow1_001:Supplay Air_Elbow_Rect:622736" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | object type "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ" | names: "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ:622088", "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ:622737" | material: "Material_Duct" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "AXC-800-9-4" | object type "AXC:AXC-800-9-4" | names: "AXC:AXC-800-9-4:622523" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | object type "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ" | names: "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ:622629", "magicirc_multi_shape_trans_001:Supplay Air_Multi shape transition_Circ:622686" | material: "Material_Duct" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | object type "magirect_elbow1_001:Supplay Air_Elbow_Rect" | names: "magirect_elbow1_001:Supplay Air_Elbow_Rect:622640", "magirect_elbow1_001:Supplay Air_Elbow_Rect:622685" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics

Types
  IFCDUCTSEGMENTTYPE "Rectangular Duct:Air" | 20 occurrences | property sets: Construction, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | 5 occurrences | property sets: Constraints, Identity Data, Other
  IFCDUCTSEGMENTTYPE "Round Duct:Air" | 18 occurrences | property sets: Construction, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Elbow short_Circ" | 2 occurrences | property sets: Constraints, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "WK25 200 200-1" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCDUCTFITTINGTYPE "Supplay Air_Elbow short_Circ" | 3 occurrences | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Tee centric 90_Circ" | 1 occurrence | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Reduction_Circ" | 1 occurrence | material: "Material_Duct" | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | 1 occurrence | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | 1 occurrence | material: "Material_Duct" | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | 1 occurrence | material: "Material_Duct" | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | 1 occurrence | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Elbow short_Circ" | 2 occurrences | property sets: Constraints, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "WK25 200 200-1" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCDUCTFITTINGTYPE "Supplay Air_Elbow short_Circ" | 3 occurrences | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Tee centric 90_Circ" | 1 occurrence | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Reduction_Circ" | 1 occurrence | material: "Material_Duct" | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | 1 occurrence | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | 1 occurrence | material: "Material_Duct" | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | 1 occurrence | material: "Material_Duct" | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Tbranch_Rect" | 1 occurrence | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | 1 occurrence | property sets: Constraints, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "AXC-800-9-4" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Pset_BuildingElementProxyCommon, Pset_ProductRequirements
  IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | 2 occurrences | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | 2 occurrences | material: "Material_Duct" | property sets: Constraints, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "AXC-800-9-4" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Pset_BuildingElementProxyCommon, Pset_ProductRequirements
  IFCDUCTFITTINGTYPE "Supplay Air_Multi shape transition_Circ" | 2 occurrences | material: "Material_Duct" | property sets: Constraints, Identity Data, Other
  IFCDUCTFITTINGTYPE "Supplay Air_Elbow_Rect" | 2 occurrences | property sets: Constraints, Identity Data, Other

Property sets
  Other | properties | on 40 objects (40 IFCFLOWSEGMENT)
    Category = "Ducts" (IFCLABEL)
    Family = "Rectangular Duct: Air" (IFCLABEL)
    Family and Type = "Rectangular Duct: Air" (IFCLABEL)
    Type = "Rectangular Duct: Air" (IFCLABEL)
    Type Id = "Rectangular Duct: Air" (IFCLABEL)
  Other | properties | on 36 objects (36 IFCFLOWSEGMENT)
    Category = "Ducts" (IFCLABEL)
    Family = "Round Duct: Air" (IFCLABEL)
    Family and Type = "Round Duct: Air" (IFCLABEL)
    Type = "Round Duct: Air" (IFCLABEL)
    Type Id = "Round Duct: Air" (IFCLABEL)
  Other | properties | on 10 objects (10 IFCFLOWFITTING)
    Category = "Duct Fittings" (IFCLABEL)
    Family = "magicirc_elbow_short_001: Supplay Air_Elbow short_Circ" (IFCLABEL)
    Family and Type = "magicirc_elbow_short_001: Supplay Air_Elbow short_Circ" (IFCLABEL)
    Type = "magicirc_elbow_short_001: Supplay Air_Elbow short_Circ" (IFCLABEL)
    Type Id = "magicirc_elbow_short_001: Supplay Air_Elbow short_Circ" (IFCLABEL)
  Other | properties | on 10 objects (10 IFCFLOWFITTING)
    Category = "Duct Fittings" (IFCLABEL)
    Family = "magirect_elbow1_001: Supplay Air_Elbow_Rect" (IFCLABEL)
    Family and Type = "magirect_elbow1_001: Supplay Air_Elbow_Rect" (IFCLABEL)
    Type = "magirect_elbow1_001: Supplay Air_Elbow_Rect" (IFCLABEL)
    Type Id = "magirect_elbow1_001: Supplay Air_Elbow_Rect" (IFCLABEL)
  Other | properties | on 8 objects (8 IFCFLOWFITTING)
    Category = "Duct Fittings" (IFCLABEL)
    Family = "magicirc_multi_shape_trans_001: Supplay Air_Multi shape transition_Circ" (IFCLABEL)
    Family and Type = "magicirc_multi_shape_trans_001: Supplay Air_Multi shape transition_Circ" (IFCLABEL)
    Type = "magicirc_multi_shape_trans_001: Supplay Air_Multi shape transition_Circ" (IFCLABEL)
    Type Id = "magicirc_multi_shape_trans_001: Supplay Air_Multi shape transition_Circ" (IFCLABEL)
    Visibility_Ins = FALSE (IFCBOOLEAN)
    Visibility_Lining = FALSE (IFCBOOLEAN)
  Other | properties | on 4 objects (4 IFCFLOWFITTING)
    Category = "Duct Fittings" (IFCLABEL)
    Family = "magirect_tbranch1_001: Supplay Air_Tbranch_Rect" (IFCLABEL)
    Family and Type = "magirect_tbranch1_001: Supplay Air_Tbranch_Rect" (IFCLABEL)
    Type = "magirect_tbranch1_001: Supplay Air_Tbranch_Rect" (IFCLABEL)
    Type Id = "magirect_tbranch1_001: Supplay Air_Tbranch_Rect" (IFCLABEL)
  Other | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCSYSTEM)
    Category = "Duct Systems" (IFCLABEL)
    Family = "Duct System: D3060.20.-ROSSZ LEVEGŐ" (IFCLABEL)
    Family and Type = "Duct System: D3060.20.-ROSSZ LEVEGŐ" (IFCLABEL)
    Type = "Duct System: D3060.20.-ROSSZ LEVEGŐ" (IFCLABEL)
    Type Id = "Duct System: D3060.20.-ROSSZ LEVEGŐ" (IFCLABEL)
  Other: 15 more contents on 10 objects not shown
  Mechanical - Flow | properties | on 32 objects (32 IFCFLOWSEGMENT)
    Additional Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Friction = 0. (IFCREAL) [derived "Friction Loss"]
    Pressure Drop = 0. (IFCPRESSUREMEASURE) [PASCAL]
    Reynolds number = 0. (IFCREAL)
    Velocity = 0. (IFCLINEARVELOCITYMEASURE) [derived]
    Velocity Pressure = 0. (IFCPRESSUREMEASURE) [PASCAL]
  Mechanical - Flow | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Additional Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow = 1.94230666968187 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Friction = 0.74026427480169 (IFCREAL) [derived "Friction Loss"]
    Pressure Drop = 0.222761450775029 (IFCPRESSUREMEASURE) [PASCAL]
    Reynolds number = 29035.4901139502 (IFCREAL)
    Velocity = 2.73547558439196 (IFCLINEARVELOCITYMEASURE) [derived]
    Velocity Pressure = 4.49949167752261 (IFCPRESSUREMEASURE) [PASCAL]
  Mechanical - Flow | properties | on 6 objects (6 IFCFLOWFITTING)
    Pressure Drop = 0. (IFCPRESSUREMEASURE) [PASCAL]
  Mechanical - Flow | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Additional Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow = 1.94230666968187 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Friction = 0.740264274801686 (IFCREAL) [derived "Friction Loss"]
    Pressure Drop = 0.171571305627863 (IFCPRESSUREMEASURE) [PASCAL]
    Reynolds number = 29035.4901139502 (IFCREAL)
    Velocity = 2.73547558439195 (IFCLINEARVELOCITYMEASURE) [derived]
    Velocity Pressure = 4.49949167752259 (IFCPRESSUREMEASURE) [PASCAL]
  Mechanical - Flow | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Additional Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow = 1.76573333607443 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Friction = 6.33059072981465 (IFCREAL) [derived "Friction Loss"]
    Pressure Drop = 10.113118690879 (IFCPRESSUREMEASURE) [PASCAL]
    Reynolds number = 42233.4401657457 (IFCREAL)
    Velocity = 6.36619772367581 (IFCLINEARVELOCITYMEASURE) [derived]
    Velocity Pressure = 24.3701393866215 (IFCPRESSUREMEASURE) [PASCAL]
  Mechanical - Flow | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Additional Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow = 1.76573333607443 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Friction = 6.33059072981468 (IFCREAL) [derived "Friction Loss"]
    Pressure Drop = 2.13291225118674 (IFCPRESSUREMEASURE) [PASCAL]
    Reynolds number = 42233.4401657457 (IFCREAL)
    Velocity = 6.36619772367582 (IFCLINEARVELOCITYMEASURE) [derived]
    Velocity Pressure = 24.3701393866216 (IFCPRESSUREMEASURE) [PASCAL]
  Mechanical - Flow | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Additional Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow = 1.94230666968187 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Friction = 0.740264274801686 (IFCREAL) [derived "Friction Loss"]
    Pressure Drop = 0.916598449519359 (IFCPRESSUREMEASURE) [PASCAL]
    Reynolds number = 29035.4901139502 (IFCREAL)
    Velocity = 2.73547558439195 (IFCLINEARVELOCITYMEASURE) [derived]
    Velocity Pressure = 4.49949167752259 (IFCPRESSUREMEASURE) [PASCAL]
  Mechanical - Flow | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Additional Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow = 1.94230666968187 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Friction = 0.740264274801686 (IFCREAL) [derived "Friction Loss"]
    Pressure Drop = 0.568701432360739 (IFCPRESSUREMEASURE) [PASCAL]
    Reynolds number = 29035.4901139502 (IFCREAL)
    Velocity = 2.73547558439195 (IFCLINEARVELOCITYMEASURE) [derived]
    Velocity Pressure = 4.49949167752259 (IFCPRESSUREMEASURE) [PASCAL]
  Mechanical - Flow: 11 more contents on 30 objects not shown
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "20" (IFCTEXT)
    Productdata = "© Progman Oy, all rights reserved" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "26" (IFCTEXT)
    Productdata = "© Progman Oy, all rights reserved" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "32" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "33" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "01 Level" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "03 Level" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "04 Roof" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data: 10 more contents on 0 objects not shown
  Constraints | properties | on 20 objects (18 IFCFLOWFITTING, 2 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: 03 Level" (IFCLABEL)
  Constraints | properties | on 16 objects (16 IFCFLOWSEGMENT)
    Bottom Elevation = 2920. (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 03 Level" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 3080. (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 12 objects (10 IFCFLOWFITTING, 2 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: 04 Roof" (IFCLABEL)
  Constraints | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Bottom Elevation = 2603.07847999999 (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 2904. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 2603.07847999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 03 Level" (IFCLABEL)
    Start Middle Elevation = 2603.07847999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 2904. (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Bottom Elevation = 2900. (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 03 Level" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 3100. (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Bottom Elevation = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 04 Roof" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 2200. (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Bottom Elevation = 1950. (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 04 Roof" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 2250. (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Bottom Elevation = 2949.99999999994 (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 2999.99999999994 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 2999.99999999994 (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 03 Level" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 2999.99999999994 (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 3049.99999999994 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints: 15 more contents on 35 objects not shown
  Dimensions | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Diameter = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 300.921520000008 (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "160 mmø" (IFCTEXT)
  Dimensions | properties | on 6 objects (6 IFCFLOWFITTING)
    Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Angle_list = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    B_Lining = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Bout = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Bout_Ins = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    H_Lining = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    Hout = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    Hout_Ins = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    L = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "200 mmx350 mm-200 mmx350 mm" (IFCTEXT)
    ThroatR = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Visibility_Ins = FALSE (IFCBOOLEAN)
    Visibility_Lining = FALSE (IFCBOOLEAN)
    Volume = 0.0219910511696922 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    rc = 200. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Height = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 2225. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "350 mmx200 mm" (IFCTEXT)
    Width = 350. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Diameter = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 231.770344008329 (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "160 mmø" (IFCTEXT)
  Dimensions | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Diameter = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 1597.50000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "100 mmø" (IFCTEXT)
  Dimensions | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Diameter = 99.9999999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 336.921519999948 (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "100 mmø" (IFCTEXT)
  Dimensions | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Diameter = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 1238.20435582267 (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "160 mmø" (IFCTEXT)
  Dimensions | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Diameter = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 768.241088647823 (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "160 mmø" (IFCTEXT)
  Dimensions: 34 more contents on 81 objects not shown
  Insulation | properties | on 24 objects (24 IFCFLOWSEGMENT)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "350 mmx200 mm" (IFCTEXT)
  Insulation | properties | on 24 objects (24 IFCFLOWSEGMENT)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "160 mmø" (IFCTEXT)
  Insulation | properties | on 12 objects (12 IFCFLOWSEGMENT)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "100 mmø" (IFCTEXT)
  Insulation | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "200 mmx200 mm" (IFCTEXT)
  Insulation | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "300 mmx300 mm" (IFCTEXT)
  Insulation | properties | on 6 objects (6 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "160 mmø-160 mmø" (IFCTEXT)
  Insulation | properties | on 6 objects (6 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "200 mmx350 mm-200 mmx350 mm" (IFCTEXT)
  Insulation | properties | on 4 objects (4 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "100 mmø-100 mmø" (IFCTEXT)
  Insulation: 12 more contents on 24 objects not shown
  Lining | properties | on 24 objects (24 IFCFLOWSEGMENT)
    Free Size = "350 mmx200 mm" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining | properties | on 24 objects (24 IFCFLOWSEGMENT)
    Free Size = "160 mmø" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining | properties | on 12 objects (12 IFCFLOWSEGMENT)
    Free Size = "100 mmø" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Free Size = "200 mmx200 mm" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining | properties | on 8 objects (8 IFCFLOWSEGMENT)
    Free Size = "300 mmx300 mm" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining | properties | on 6 objects (6 IFCFLOWFITTING)
    Free Size = "160 mmø-160 mmø" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining | properties | on 6 objects (6 IFCFLOWFITTING)
    Free Size = "200 mmx350 mm-200 mmx350 mm" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining | properties | on 4 objects (4 IFCFLOWFITTING)
    Free Size = "100 mmø-100 mmø" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Lining: 12 more contents on 24 objects not shown
  Mechanical | properties | on 3 objects (3 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Method = "8baf7d75-8b9b-46d0-b8ce-3ad1c19e6b19" (IFCTEXT)
    MC_B = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    MC_H = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    System Abbreviation = "RL" (IFCTEXT)
    System Classification = "Return Air" (IFCTEXT)
    System Name = "Mechanical D3060.20.-ROSSZ LEVEGŐ 1" (IFCTEXT)
    System Type = "Duct System: D3060.20.-ROSSZ LEVEGŐ" (IFCLABEL)
  Mechanical | properties | on 3 objects (3 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Method = "8baf7d75-8b9b-46d0-b8ce-3ad1c19e6b19" (IFCTEXT)
    MC_B = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    MC_H = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    System Abbreviation = "RL" (IFCTEXT)
    System Classification = "Return Air" (IFCTEXT)
    System Name = "Mechanical D3060.20.-ROSSZ LEVEGŐ 15" (IFCTEXT)
    System Type = "Duct System: D3060.20.-ROSSZ LEVEGŐ" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 2.4475 (IFCAREAMEASURE) [SQUARE_METRE]
    Equivalent Diameter = 286.443488979839 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydraulic Diameter = 254.545454545455 (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Coefficient = 0. (IFCREAL)
    Section = 12 (IFCINTEGER)
    Size Lock = FALSE (IFCBOOLEAN)
    System Abbreviation = "RL" (IFCTEXT)
    System Classification = "Return Air" (IFCTEXT)
    System Name = "Mechanical D3060.20.-ROSSZ LEVEGŐ 1" (IFCTEXT)
    System Type = "Duct System: D3060.20.-ROSSZ LEVEGŐ" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 0.116500481609047 (IFCAREAMEASURE) [SQUARE_METRE]
    Equivalent Diameter = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydraulic Diameter = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Coefficient = 0.0381312641347811 (IFCREAL)
    Section = 29 (IFCINTEGER)
    Size Lock = FALSE (IFCBOOLEAN)
    System Abbreviation = "RL" (IFCTEXT)
    System Classification = "Return Air" (IFCTEXT)
    System Name = "Mechanical D3060.20.-ROSSZ LEVEGŐ 1" (IFCTEXT)
    System Type = "Duct System: D3060.20.-ROSSZ LEVEGŐ" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 0.501869426410974 (IFCAREAMEASURE) [SQUARE_METRE]
    Equivalent Diameter = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydraulic Diameter = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Coefficient = 0.414979928117719 (IFCREAL)
    Section = 28 (IFCINTEGER)
    Size Lock = FALSE (IFCBOOLEAN)
    System Abbreviation = "RL" (IFCTEXT)
    System Classification = "Return Air" (IFCTEXT)
    System Name = "Mechanical D3060.20.-ROSSZ LEVEGŐ 1" (IFCTEXT)
    System Type = "Duct System: D3060.20.-ROSSZ LEVEGŐ" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 0.105847017206814 (IFCAREAMEASURE) [SQUARE_METRE]
    Equivalent Diameter = 99.9999999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydraulic Diameter = 99.9999999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Coefficient = 0.0875215450083819 (IFCREAL)
    Section = 28 (IFCINTEGER)
    Size Lock = FALSE (IFCBOOLEAN)
    System Abbreviation = "RL" (IFCTEXT)
    System Classification = "Return Air" (IFCTEXT)
    System Name = "Mechanical D3060.20.-ROSSZ LEVEGŐ 1" (IFCTEXT)
    System Type = "Duct System: D3060.20.-ROSSZ LEVEGŐ" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Method = "8baf7d75-8b9b-46d0-b8ce-3ad1c19e6b19" (IFCTEXT)
    MC_R = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    System Abbreviation = "RL" (IFCTEXT)
    System Classification = "Return Air" (IFCTEXT)
    System Name = "Mechanical D3060.20.-ROSSZ LEVEGŐ 1" (IFCTEXT)
    System Type = "Duct System: D3060.20.-ROSSZ LEVEGŐ" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 0.151259653846256 (IFCAREAMEASURE) [SQUARE_METRE]
    Equivalent Diameter = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydraulic Diameter = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Coefficient = 0.0495081370830937 (IFCREAL)
    Section = 29 (IFCINTEGER)
    Size Lock = FALSE (IFCBOOLEAN)
    System Abbreviation = "RL" (IFCTEXT)
    System Classification = "Return Air" (IFCTEXT)
    System Name = "Mechanical D3060.20.-ROSSZ LEVEGŐ 1" (IFCTEXT)
    System Type = "Duct System: D3060.20.-ROSSZ LEVEGŐ" (IFCLABEL)
  Mechanical: 62 more contents on 100 objects not shown
  Phasing | properties | on 116 objects (76 IFCFLOWSEGMENT, 36 IFCFLOWFITTING, 4 IFCBUILDINGELEMENTPROXY)
    Phase Created = "Phase 1" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 38 objects (38 IFCFLOWSEGMENT)
    Reference = "Air" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 10 objects (10 IFCFLOWFITTING)
    Reference = "Supplay Air_Elbow short_Circ" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 10 objects (10 IFCFLOWFITTING)
    Reference = "Supplay Air_Elbow_Rect" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 8 objects (8 IFCFLOWFITTING)
    Reference = "Supplay Air_Multi shape transition_Circ" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 4 objects (4 IFCFLOWFITTING)
    Reference = "Supplay Air_Tbranch_Rect" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 2 objects (2 IFCFLOWFITTING)
    Reference = "Supplay Air_Tee centric 90_Circ" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 2 objects (2 IFCFLOWFITTING)
    Reference = "Supplay Air_Reduction_Circ" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 38 objects (38 IFCFLOWSEGMENT)
    Roughness = 0.150000005960465 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Length = 300.921520000008 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 2225. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 231.770344008329 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 1597.50000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 336.921519999948 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 1238.20435582267 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 768.241088647823 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 179.671447124557 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment: 14 more contents on 20 objects not shown
  Pset_FlowSegmentPipeSegment | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Length = 300.921520000008 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 2225. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 231.770344008329 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 1597.50000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 336.921519999948 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 1238.20435582267 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 768.241088647823 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 179.671447124557 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment: 14 more contents on 20 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 20 objects (20 IFCFLOWSEGMENT)
    Manufacturer = "Generic" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 18 objects (18 IFCFLOWSEGMENT)
    Manufacturer (no value)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Manufacturer = "Lindab" (IFCLABEL)
  Pset_ProductRequirements | properties | on 38 objects (38 IFCFLOWSEGMENT)
    Category = "Ducts" (IFCLABEL)
  Pset_ProductRequirements | properties | on 36 objects (36 IFCFLOWFITTING)
    Category = "Duct Fittings" (IFCLABEL)
  Pset_ProductRequirements | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY) | on 4 type objects
    Category = "Duct Accessories" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "01 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "03 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "04 Roof" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 38 objects (38 IFCFLOWSEGMENT)
    Reference = "Air" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 10 objects (10 IFCFLOWFITTING)
    Reference = "Supplay Air_Elbow short_Circ" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 10 objects (10 IFCFLOWFITTING)
    Reference = "Supplay Air_Elbow_Rect" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 8 objects (8 IFCFLOWFITTING)
    Reference = "Supplay Air_Multi shape transition_Circ" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCFLOWFITTING)
    Reference = "Supplay Air_Tbranch_Rect" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "WK25 200 200-1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "AXC-800-9-4" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCFLOWFITTING)
    Reference = "Supplay Air_Tee centric 90_Circ" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 1 more content on 2 objects not shown
  Graphics | properties | on 30 objects (26 IFCFLOWFITTING, 4 IFCBUILDINGELEMENTPROXY)
    Use Annotation Scale = FALSE (IFCBOOLEAN)
  Graphics | properties | on 10 objects (10 IFCFLOWFITTING)
    Segmented = FALSE (IFCBOOLEAN)
    SubTp = 2 (IFCINTEGER)
    Use Annotation Scale = FALSE (IFCBOOLEAN)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "WK25 200 200-1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "AXC-800-9-4" (IFCIDENTIFIER)
  Materials and Finishes | properties | on 10 objects (10 IFCFLOWFITTING)
    Material_Duct = "Material_Duct" (IFCLABEL)
    Material_Ins = "Material_Ins" (IFCLABEL)
    Material_Lining = "Material_Lining" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "01 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "03 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "04 Roof" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 3 (IFCINTEGER)
  Constraints(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Other(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Construction | properties | on 2 type objects
    Roughness = 0.150000005960465 (IFCLENGTHMEASURE) [MILLI METRE]

Other addresses and roles
  2 x postal address: "Enter address here", "Boston", "MA"