IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "0001"
Time stamp: "2021-05-09T13:23:45"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190327_2315(x64) - Exporter 20.0.0.377 - Alternate UI 20.0.0.377"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "jozsef.etlinger" of Organization (no name given)
  Owner history of Person "jozsef.etlinger" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1620559188 (2021-05-09T11:19:48Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "00 Ground level" | long name "00 Ground level" | object type "Level:8mm Head" | elevation 0.
        contains 15 elements
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:01_Belső kerámia fal 300 mm+vakolat" | object type "Basic Wall:01_Belső kerámia fal 300 mm+vakolat" | names: "Basic Wall:01_Belső kerámia fal 300 mm+vakolat:394695", "Basic Wall:01_Belső kerámia fal 300 mm+vakolat:417421", "Basic Wall:01_Belső kerámia fal 300 mm+vakolat:417779" | material: layers "Basic Wall:01_Belső kerámia fal 300 mm+vakolat" ("03_Vakolat" 10., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          12 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" | object type "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" | names: "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton:394696", "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton:394697", "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton:394698" (+9 more) | material: layers "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" ("03_Normál gipszkarton építőlemez" 12.5, "04_Üveggyapot - Akustik Board" 75., "03_Normál gipszkarton építőlemez" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
      IFCBUILDINGSTOREY "01 Level" | long name "01 Level" | object type "Level:8mm Head" | elevation 4000.
        contains 37 elements
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" | object type "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" | names: "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton:388617", "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton:388620", "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton:388676" (+1 more) | material: layers "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" ("03_Normál gipszkarton építőlemez" 12.5, "03_Normál gipszkarton építőlemez" 12.5, "04_Üveggyapot - Akustik Board" 100., "03_Normál gipszkarton építőlemez" 12.5, "03_Normál gipszkarton építőlemez" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:01_Belső kerámia fal 300 mm+vakolat" | object type "Basic Wall:01_Belső kerámia fal 300 mm+vakolat" | names: "Basic Wall:01_Belső kerámia fal 300 mm+vakolat:388618", "Basic Wall:01_Belső kerámia fal 300 mm+vakolat:388619", "Basic Wall:01_Belső kerámia fal 300 mm+vakolat:388677" | material: layers "Basic Wall:01_Belső kerámia fal 300 mm+vakolat" ("03_Vakolat" 10., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" | object type "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" | names: "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton:388621", "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton:388622", "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton:388623" (+7 more) | material: layers "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" ("03_Normál gipszkarton építőlemez" 12.5, "04_Üveggyapot - Akustik Board" 75., "03_Normál gipszkarton építőlemez" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          20 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:01_Belső kerámia burkolat" | object type "Basic Wall:01_Belső kerámia burkolat" | names: "Basic Wall:01_Belső kerámia burkolat:415908", "Basic Wall:01_Belső kerámia burkolat:415983", "Basic Wall:01_Belső kerámia burkolat:416048" (+17 more) | material: layers "Basic Wall:01_Belső kerámia burkolat" ("07_Kerámia lapburkolat" 15., "06_Gyorskötésű burkolatragasztó" 5.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
      IFCBUILDINGSTOREY "02 Level" | long name "02 Level" | object type "Level:8mm Head" | elevation 8000.
        contains 37 elements
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" | object type "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" | names: "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton:389887", "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton:389890", "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton:389946" (+1 more) | material: layers "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" ("03_Normál gipszkarton építőlemez" 12.5, "03_Normál gipszkarton építőlemez" 12.5, "04_Üveggyapot - Akustik Board" 100., "03_Normál gipszkarton építőlemez" 12.5, "03_Normál gipszkarton építőlemez" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:01_Belső kerámia fal 300 mm+vakolat" | object type "Basic Wall:01_Belső kerámia fal 300 mm+vakolat" | names: "Basic Wall:01_Belső kerámia fal 300 mm+vakolat:389888", "Basic Wall:01_Belső kerámia fal 300 mm+vakolat:389889", "Basic Wall:01_Belső kerámia fal 300 mm+vakolat:389947" | material: layers "Basic Wall:01_Belső kerámia fal 300 mm+vakolat" ("03_Vakolat" 10., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" | object type "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" | names: "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton:389891", "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton:389892", "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton:389893" (+7 more) | material: layers "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" ("03_Normál gipszkarton építőlemez" 12.5, "04_Üveggyapot - Akustik Board" 75., "03_Normál gipszkarton építőlemez" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          20 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:01_Belső kerámia burkolat" | object type "Basic Wall:01_Belső kerámia burkolat" | names: "Basic Wall:01_Belső kerámia burkolat:416500", "Basic Wall:01_Belső kerámia burkolat:416501", "Basic Wall:01_Belső kerámia burkolat:416502" (+17 more) | material: layers "Basic Wall:01_Belső kerámia burkolat" ("07_Kerámia lapburkolat" 15., "06_Gyorskötésű burkolatragasztó" 5.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
      IFCBUILDINGSTOREY "03 Level" | long name "03 Level" | object type "Level:8mm Head" | elevation 12000.
        contains 37 elements
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" | object type "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" | names: "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton:391157", "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton:391160", "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton:391216" (+1 more) | material: layers "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" ("03_Normál gipszkarton építőlemez" 12.5, "03_Normál gipszkarton építőlemez" 12.5, "04_Üveggyapot - Akustik Board" 100., "03_Normál gipszkarton építőlemez" 12.5, "03_Normál gipszkarton építőlemez" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:01_Belső kerámia fal 300 mm+vakolat" | object type "Basic Wall:01_Belső kerámia fal 300 mm+vakolat" | names: "Basic Wall:01_Belső kerámia fal 300 mm+vakolat:391158", "Basic Wall:01_Belső kerámia fal 300 mm+vakolat:391159", "Basic Wall:01_Belső kerámia fal 300 mm+vakolat:391217" | material: layers "Basic Wall:01_Belső kerámia fal 300 mm+vakolat" ("03_Vakolat" 10., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" | object type "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" | names: "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton:391161", "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton:391162", "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton:391163" (+7 more) | material: layers "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" ("03_Normál gipszkarton építőlemez" 12.5, "04_Üveggyapot - Akustik Board" 75., "03_Normál gipszkarton építőlemez" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          20 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:01_Belső kerámia burkolat" | object type "Basic Wall:01_Belső kerámia burkolat" | names: "Basic Wall:01_Belső kerámia burkolat:416521", "Basic Wall:01_Belső kerámia burkolat:416522", "Basic Wall:01_Belső kerámia burkolat:416523" (+17 more) | material: layers "Basic Wall:01_Belső kerámia burkolat" ("07_Kerámia lapburkolat" 15., "06_Gyorskötésű burkolatragasztó" 5.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing

Types
  IFCWALLTYPE "Basic Wall:01_Belső kerámia fal 300 mm+vakolat" | STANDARD | 12 occurrences | material: layers "Basic Wall:01_Belső kerámia fal 300 mm+vakolat" ("03_Vakolat" 10., "02_Porotherm 30 N+F tégla" 300., "03_Vakolat" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" | STANDARD | 42 occurrences | material: layers "Basic Wall:01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" ("03_Normál gipszkarton építőlemez" 12.5, "04_Üveggyapot - Akustik Board" 75., "03_Normál gipszkarton építőlemez" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" | STANDARD | 12 occurrences | material: layers "Basic Wall:01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" ("03_Normál gipszkarton építőlemez" 12.5, "03_Normál gipszkarton építőlemez" 12.5, "04_Üveggyapot - Akustik Board" 100., "03_Normál gipszkarton építőlemez" 12.5, "03_Normál gipszkarton építőlemez" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:01_Belső kerámia burkolat" | STANDARD | 60 occurrences | material: layers "Basic Wall:01_Belső kerámia burkolat" ("07_Kerámia lapburkolat" 15., "06_Gyorskötésű burkolatragasztó" 5.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other

Property sets
  Other | properties | on 60 objects (60 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: 01_Belső kerámia burkolat" (IFCLABEL)
    Family and Type = "Basic Wall: 01_Belső kerámia burkolat" (IFCLABEL)
    Type = "Basic Wall: 01_Belső kerámia burkolat" (IFCLABEL)
    Type Id = "Basic Wall: 01_Belső kerámia burkolat" (IFCLABEL)
  Other | properties | on 42 objects (42 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: 01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" (IFCLABEL)
    Family and Type = "Basic Wall: 01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" (IFCLABEL)
    Type = "Basic Wall: 01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" (IFCLABEL)
    Type Id = "Basic Wall: 01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" (IFCLABEL)
  Other | properties | on 12 objects (12 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: 01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" (IFCLABEL)
    Family and Type = "Basic Wall: 01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" (IFCLABEL)
    Type = "Basic Wall: 01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" (IFCLABEL)
    Type Id = "Basic Wall: 01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" (IFCLABEL)
  Other | properties | on 12 objects (12 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: 01_Belső kerámia fal 300 mm+vakolat" (IFCLABEL)
    Family and Type = "Basic Wall: 01_Belső kerámia fal 300 mm+vakolat" (IFCLABEL)
    Type = "Basic Wall: 01_Belső kerámia fal 300 mm+vakolat" (IFCLABEL)
    Type Id = "Basic Wall: 01_Belső kerámia fal 300 mm+vakolat" (IFCLABEL)
  Other | properties | on 12 objects (12 IFCOPENINGELEMENT)
    Category = "Doors" (IFCLABEL)
    Family = "M_Single-Flush: 750 x 2100mm" (IFCLABEL)
    Family and Type = "M_Single-Flush: 750 x 2100mm" (IFCLABEL)
    Head Height = 1960. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: 01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" (IFCLABEL)
    Küszöb = TRUE (IFCBOOLEAN)
    Takaró = TRUE (IFCBOOLEAN)
    Type = "M_Single-Flush: 750 x 2100mm" (IFCLABEL)
    Type Id = "M_Single-Flush: 750 x 2100mm" (IFCLABEL)
  Other | properties | on 8 objects (8 IFCOPENINGELEMENT)
    Category = "Rectangular Straight Wall Opening" (IFCLABEL)
  Other | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other: 1 more content on 0 objects not shown
  BaseQuantities | quantities | on 18 objects (18 IFCOPENINGELEMENT)
    Depth = 3048. [MILLI METRE]
    Height = 2240. [MILLI METRE]
    Width = 750.000000000003 [MILLI METRE]
  BaseQuantities | quantities | on 14 objects (14 IFCOPENINGELEMENT)
    Depth = 3048. [MILLI METRE]
    Height = 2240. [MILLI METRE]
    Width = 900.000000000003 [MILLI METRE]
  BaseQuantities | quantities | on 8 objects (8 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 0.0999999999999948 [SQUARE_METRE]
    Height = 3800. [MILLI METRE]
    Length = 1000. [MILLI METRE]
    NetSideArea = 3.80000000000001 [SQUARE_METRE]
    NetSideArea = 3800000.00000001 [SQUARE_METRE]
    NetVolume = 0.380000000000013 [CUBIC_METRE]
    NetVolume = 380000000.000001 [CUBIC_METRE]
    Width = 100. [MILLI METRE]
  BaseQuantities | quantities | on 8 objects (8 IFCOPENINGELEMENT)
    Depth = 3048. [MILLI METRE]
    Height = 900.000000000003 [MILLI METRE]
    Width = 2240. [MILLI METRE]
  BaseQuantities | quantities | on 6 objects (6 IFCOPENINGELEMENT)
    Depth = 150.000000000001 [MILLI METRE]
    Height = 1700. [MILLI METRE]
    Width = 2240. [MILLI METRE]
  BaseQuantities | quantities | on 6 objects (6 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 0.0195999999999955 [SQUARE_METRE]
    Height = 2100. [MILLI METRE]
    Length = 979.999999999998 [MILLI METRE]
    NetSideArea = 2.058 [SQUARE_METRE]
    NetSideArea = 2058000. [SQUARE_METRE]
    NetVolume = 0.0411600000000084 [CUBIC_METRE]
    NetVolume = 41159999.9999999 [CUBIC_METRE]
    Width = 20. [MILLI METRE]
  BaseQuantities | quantities | on 6 objects (6 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 0.0195999999999953 [SQUARE_METRE]
    Height = 2100. [MILLI METRE]
    Length = 979.999999999989 [MILLI METRE]
    NetSideArea = 2.05799999999998 [SQUARE_METRE]
    NetSideArea = 2057999.99999998 [SQUARE_METRE]
    NetVolume = 0.041160000000008 [CUBIC_METRE]
    NetVolume = 41159999.9999995 [CUBIC_METRE]
    Width = 20. [MILLI METRE]
  BaseQuantities | quantities | on 6 objects (6 IFCOPENINGELEMENT)
    Depth = 3048. [MILLI METRE]
    Height = 750.000000000003 [MILLI METRE]
    Width = 2240. [MILLI METRE]
  BaseQuantities: 56 more contents on 110 objects not shown
  Constraints | properties | on 20 objects (20 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: 01 Level" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 01 Level" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 20 objects (20 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: 02 Level" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 02 Level" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 20 objects (20 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: 03 Level" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 03 Level" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 17 objects (17 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: 01 Level" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -140. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Interior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 02 Level" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = -340. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 3800. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 17 objects (17 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: 02 Level" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -140. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Interior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 03 Level" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = -340. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 3800. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 17 objects (17 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: 03 Level" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -140. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Interior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 04 Roof" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = -340. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 3800. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 15 objects (15 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: 00 Ground level" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -140. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Interior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 01 Level" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = -340. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 3800. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 4 objects (4 IFCOPENINGELEMENT)
    Level = "Level: 01 Level" (IFCLABEL)
    Sill Height = -140. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints: 10 more contents on 20 objects not shown
  Dimensions | properties | on 12 objects (12 IFCOPENINGELEMENT)
    Area = 2.71394999999998 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.105759999999999 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    m = 140. (IFCLENGTHMEASURE) [MILLI METRE]
    m1 = 140. (IFCLENGTHMEASURE) [MILLI METRE]
    m2 = 140. (IFCLENGTHMEASURE) [MILLI METRE]
    sz = 125.000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 8 objects (8 IFCWALLSTANDARDCASE)
    Area = 3.80000000000001 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 1100. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.380000000000013 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 6 objects (6 IFCWALLSTANDARDCASE)
    Area = 2.058 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 979.999999999994 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0411600000000084 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 6 objects (6 IFCWALLSTANDARDCASE)
    Area = 2.05799999999998 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 979.999999999994 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.041160000000008 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Area = 2.45174999999999 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 1167.49999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0490350000000098 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 3 objects (3 IFCWALLSTANDARDCASE)
    Area = 13.3000000000001 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3880.00000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.99500000000002 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 3 objects (3 IFCWALLSTANDARDCASE)
    Area = 21.238 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 7030. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 6.79616000000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 48 more contents on 96 objects not shown
  Identity Data | properties | on 126 objects (126 IFCWALLSTANDARDCASE)
    Comments = "Belső fal" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCOPENINGELEMENT)
    Comments = "Nyílászáró" (IFCTEXT)
    Mark = "44" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCOPENINGELEMENT)
    Comments = "Nyílászáró" (IFCTEXT)
    Mark = "47" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCOPENINGELEMENT)
    Comments = "Nyílászáró" (IFCTEXT)
    Mark = "43" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCOPENINGELEMENT)
    Comments = "Nyílászáró" (IFCTEXT)
    Mark = "46" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCOPENINGELEMENT)
    Comments = "Nyílászáró" (IFCTEXT)
    Mark = "77" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCOPENINGELEMENT)
    Comments = "Nyílászáró" (IFCTEXT)
    Mark = "80" (IFCTEXT)
  Identity Data: 14 more contents on 10 objects not shown
  Phasing | properties | on 146 objects (126 IFCWALLSTANDARDCASE, 20 IFCOPENINGELEMENT)
    Phase Created = "Phase 1" (IFCLABEL)
  Structural | properties | on 126 objects (126 IFCWALLSTANDARDCASE)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 146 objects (126 IFCWALLSTANDARDCASE, 20 IFCOPENINGELEMENT) | on 4 type objects
    Roughness = 914.4 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProductRequirements | properties | on 146 objects (126 IFCWALLSTANDARDCASE, 20 IFCOPENINGELEMENT) | on 4 type objects
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "00 Ground level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "01 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "02 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "03 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 72 objects (60 IFCWALLSTANDARDCASE, 12 IFCOPENINGELEMENT) | on 1 type object
    Reference = "01_Belső kerámia burkolat" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 42 objects (42 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 18 objects (12 IFCWALLSTANDARDCASE, 6 IFCOPENINGELEMENT) | on 1 type object
    Reference = "01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 14 objects (12 IFCWALLSTANDARDCASE, 2 IFCOPENINGELEMENT) | on 1 type object
    Reference = "01_Belső kerámia fal 300 mm+vakolat" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfWall | properties | on 60 objects (60 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "01_Belső kerámia burkolat" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 42 objects (42 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 12 objects (12 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 12 objects (12 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "01_Belső kerámia fal 300 mm+vakolat" (IFCLABEL)
  Pset_WallCommon | properties | on 60 objects (60 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "01_Belső kerámia burkolat" (IFCIDENTIFIER)
    ThermalTransmittance = 45.2830188679245 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 42 objects (42 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" (IFCIDENTIFIER)
    ThermalTransmittance = 0.586466165413534 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 12 objects (12 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" (IFCIDENTIFIER)
    ThermalTransmittance = 0.434944237918216 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 12 objects (12 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "01_Belső kerámia fal 300 mm+vakolat" (IFCIDENTIFIER)
    ThermalTransmittance = 0.628029969149405 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "01_Belső kerámia fal 300 mm+vakolat" (IFCIDENTIFIER)
    ThermalTransmittance = 0.628029969149405 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "01_Belső gipszkarton fal 100 mm - 1 réteg gipszkarton" (IFCIDENTIFIER)
    ThermalTransmittance = 0.586466165413534 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" (IFCIDENTIFIER)
    ThermalTransmittance = 0.434944237918216 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "01_Belső kerámia burkolat" (IFCIDENTIFIER)
    ThermalTransmittance = 45.2830188679245 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_OpeningElementCommon | properties | on 12 objects (12 IFCOPENINGELEMENT)
    Reference = "01_Belső kerámia burkolat" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 6 objects (6 IFCOPENINGELEMENT)
    Reference = "01_Belső gipszkarton fal 150 mm - 2 réteg gipszkarton" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 2 objects (2 IFCOPENINGELEMENT)
    Reference = "01_Belső kerámia fal 300 mm+vakolat" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "00 Ground level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "01 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "02 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "03 Level" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 4 (IFCINTEGER)
  Analytical Properties(Type) | properties | on 12 objects (12 IFCOPENINGELEMENT)
    Analytic Construction = "Metal" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
    Heat Transfer Coefficient (U) = 3.7021 (IFCREAL)
    Solar Heat Gain Coefficient = 0. (IFCREAL)
    Thermal Resistance (R) = 0.270116960643959 (IFCREAL)
    Visual Light Transmittance = 0. (IFCREAL)
  Construction(Type) | properties | on 12 objects (12 IFCOPENINGELEMENT)
    Function = "Interior" (IFCIDENTIFIER)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Dimensions(Type) | properties | on 12 objects (12 IFCOPENINGELEMENT)
    Height = 2100. (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 51. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Projection Ext = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Projection Int = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Width = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 750. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data(Type) | properties | on 12 objects (12 IFCOPENINGELEMENT)
    Assembly Code = "C1020300" (IFCTEXT)
    Assembly Description = "Interior Doors with Frames" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "23.30.10.00" (IFCTEXT)
    OmniClass Title = "Doors" (IFCTEXT)
    Type Comments = "AJ-02" (IFCTEXT)
    Type Mark = "24" (IFCTEXT)
    Type Name = "750 x 2100mm" (IFCTEXT)
  Identity Data(Type) | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Materials and Finishes(Type) | properties | on 12 objects (12 IFCOPENINGELEMENT)
    Door Material = "Door - Panel" (IFCLABEL)
    Frame Material = "Door - Frame" (IFCLABEL)
    mat = "Door - Frame" (IFCLABEL)
  Other(Type) | properties | on 12 objects (12 IFCOPENINGELEMENT)
    Category = "Doors" (IFCLABEL)
    Family Name = "M_Single-Flush" (IFCTEXT)
  Other(Type) | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Constraints(Type) | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.628029969149405 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 1.59228070175439 (IFCREAL)
    Thermal mass = 422520. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.586466165413534 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 1.70512820512821 (IFCREAL)
    Thermal mass = 25635.75 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.434944237918216 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 2.2991452991453 (IFCREAL)
    Thermal mass = 49581. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 45.2830188679245 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 0.0220833333333333 (IFCREAL)
    Thermal mass = 29655. (IFCREAL)
  Construction | properties | on 1 type object
    Function = "Interior" (IFCIDENTIFIER)
    Width = 320. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "Exterior" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Interior" (IFCIDENTIFIER)
    Width = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "Exterior" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Interior" (IFCIDENTIFIER)
    Width = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "Exterior" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "Exterior" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Graphics | properties | on 4 type objects
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Materials and Finishes | properties | on 2 type objects
    Structural Material = "04_Üveggyapot - Akustik Board" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Structural Material = "02_Porotherm 30 N+F tégla" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Structural Material = "06_Gyorskötésű burkolatragasztó" (IFCLABEL)

Other addresses and roles
  2 x postal address: "Enter address here", "Boston", "MA"