IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "0001"
Time stamp: "2021-05-09T13:35:00"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190327_2315(x64) - Exporter 20.0.0.377 - Alternate UI 20.0.0.377"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "jozsef.etlinger" of Organization (no name given)
  Owner history of Person "jozsef.etlinger" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1620559188 (2021-05-09T11:19:48Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "01 Level" | long name "01 Level" | object type "Level:8mm Head" | elevation 4000.
        contains 36 elements
          4 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Feketeacél cső" | object type "Pipe Types:Feketeacél cső" | names: "Pipe Types:Feketeacél cső:461303", "Pipe Types:Feketeacél cső:476361", "Pipe Types:Feketeacél cső:600585" (+1 more) | property sets: Constraints, Dimensions, Insulation, Mechanical, Mechanical - Flow, Other
          3 x IFCFLOWCONTROLLER | type IFCVALVETYPE "AT3600-50" | object type "AT3600-0001:AT3600-50" | names: "AT3600-0001:AT3600-50:475219", "AT3600-0001:AT3600-50:559568", "AT3600-0001:AT3600-50:559602" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          18 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:PE - K1" | object type "Pipe Types:PE - K1" | names: "Pipe Types:PE - K1:550307", "Pipe Types:PE - K1:550349", "Pipe Types:PE - K1:559570" (+15 more) | property sets: Constraints, Dimensions, Identity Data, Insulation, Mechanical, Mechanical - Flow
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "321G-4010-50" | object type "321G-0001:321G-4010-50" | names: "321G-0001:321G-4010-50:559652" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Sanitary Sewerage Piping_Bend" | object type "pehd_bend_001:Sanitary Sewerage Piping_Bend" | names: "pehd_bend_001:Sanitary Sewerage Piping_Bend:559782", "pehd_bend_001:Sanitary Sewerage Piping_Bend:559936", "pehd_bend_001:Sanitary Sewerage Piping_Bend:611927" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "magi_pipe_fe_tee_centric_90_001" | object type "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001" | names: "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001:559928" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          3 x IFCFLOWCONTROLLER | type IFCVALVETYPE "AT3600-50" | object type "AT3600-0001:AT3600-50" | names: "AT3600-0001:AT3600-50:600588", "AT3600-0001:AT3600-50:600708", "AT3600-0001:AT3600-50:600714" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "321G-4010-50" | object type "321G-0001:321G-4010-50" | names: "321G-0001:321G-4010-50:600720" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Sanitary Sewerage Piping_Bend" | object type "pehd_bend_001:Sanitary Sewerage Piping_Bend" | names: "pehd_bend_001:Sanitary Sewerage Piping_Bend:600723" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "magi_pipe_pex_tee_centric_90_001" | object type "magi_pipe_pex_tee_centric_90_001:magi_pipe_pex_tee_centric_90_001" | names: "magi_pipe_pex_tee_centric_90_001:magi_pipe_pex_tee_centric_90_001:611919" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
      IFCBUILDINGSTOREY "02 Level" | long name "02 Level" | object type "Level:8mm Head" | elevation 8000.
        contains 28 elements
          4 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Feketeacél cső" | object type "Pipe Types:Feketeacél cső" | names: "Pipe Types:Feketeacél cső:603886", "Pipe Types:Feketeacél cső:603892", "Pipe Types:Feketeacél cső:604850" (+1 more) | property sets: Constraints, Dimensions, Insulation, Mechanical, Mechanical - Flow, Other
          3 x IFCFLOWCONTROLLER | type IFCVALVETYPE "AT3600-50" | object type "AT3600-0001:AT3600-50" | names: "AT3600-0001:AT3600-50:603889", "AT3600-0001:AT3600-50:604009", "AT3600-0001:AT3600-50:604015" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          10 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:PE - K1" | object type "Pipe Types:PE - K1" | names: "Pipe Types:PE - K1:604004", "Pipe Types:PE - K1:604010", "Pipe Types:PE - K1:604016" (+7 more) | property sets: Constraints, Dimensions, Identity Data, Insulation, Mechanical, Mechanical - Flow
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "321G-4010-50" | object type "321G-0001:321G-4010-50" | names: "321G-0001:321G-4010-50:604021" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Sanitary Sewerage Piping_Bend" | object type "pehd_bend_001:Sanitary Sewerage Piping_Bend" | names: "pehd_bend_001:Sanitary Sewerage Piping_Bend:604024", "pehd_bend_001:Sanitary Sewerage Piping_Bend:611939", "pehd_bend_001:Sanitary Sewerage Piping_Bend:611975" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          3 x IFCFLOWCONTROLLER | type IFCVALVETYPE "AT3600-50" | object type "AT3600-0001:AT3600-50" | names: "AT3600-0001:AT3600-50:604853", "AT3600-0001:AT3600-50:604973", "AT3600-0001:AT3600-50:604979" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "321G-4010-50" | object type "321G-0001:321G-4010-50" | names: "321G-0001:321G-4010-50:604985" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Sanitary Sewerage Piping_Bend" | object type "pehd_bend_001:Sanitary Sewerage Piping_Bend" | names: "pehd_bend_001:Sanitary Sewerage Piping_Bend:604988" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "magi_pipe_pex_tee_centric_90_001" | object type "magi_pipe_pex_tee_centric_90_001:magi_pipe_pex_tee_centric_90_001" | names: "magi_pipe_pex_tee_centric_90_001:magi_pipe_pex_tee_centric_90_001:611931", "magi_pipe_pex_tee_centric_90_001:magi_pipe_pex_tee_centric_90_001:611967" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
      IFCBUILDINGSTOREY "03 Level" | long name "03 Level" | object type "Level:8mm Head" | elevation 12000.
        contains 28 elements
          4 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Feketeacél cső" | object type "Pipe Types:Feketeacél cső" | names: "Pipe Types:Feketeacél cső:606012", "Pipe Types:Feketeacél cső:606018", "Pipe Types:Feketeacél cső:610275" (+1 more) | property sets: Constraints, Dimensions, Insulation, Mechanical, Mechanical - Flow, Other
          3 x IFCFLOWCONTROLLER | type IFCVALVETYPE "AT3600-50" | object type "AT3600-0001:AT3600-50" | names: "AT3600-0001:AT3600-50:606015", "AT3600-0001:AT3600-50:606135", "AT3600-0001:AT3600-50:606141" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          10 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:PE - K1" | object type "Pipe Types:PE - K1" | names: "Pipe Types:PE - K1:606130", "Pipe Types:PE - K1:606136", "Pipe Types:PE - K1:606142" (+7 more) | property sets: Constraints, Dimensions, Identity Data, Insulation, Mechanical, Mechanical - Flow
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "321G-4010-50" | object type "321G-0001:321G-4010-50" | names: "321G-0001:321G-4010-50:606147" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Sanitary Sewerage Piping_Bend" | object type "pehd_bend_001:Sanitary Sewerage Piping_Bend" | names: "pehd_bend_001:Sanitary Sewerage Piping_Bend:606150", "pehd_bend_001:Sanitary Sewerage Piping_Bend:611987", "pehd_bend_001:Sanitary Sewerage Piping_Bend:612023" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          3 x IFCFLOWCONTROLLER | type IFCVALVETYPE "AT3600-50" | object type "AT3600-0001:AT3600-50" | names: "AT3600-0001:AT3600-50:610278", "AT3600-0001:AT3600-50:610398", "AT3600-0001:AT3600-50:610404" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "321G-4010-50" | object type "321G-0001:321G-4010-50" | names: "321G-0001:321G-4010-50:610410" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Sanitary Sewerage Piping_Bend" | object type "pehd_bend_001:Sanitary Sewerage Piping_Bend" | names: "pehd_bend_001:Sanitary Sewerage Piping_Bend:610413" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "magi_pipe_pex_tee_centric_90_001" | object type "magi_pipe_pex_tee_centric_90_001:magi_pipe_pex_tee_centric_90_001" | names: "magi_pipe_pex_tee_centric_90_001:magi_pipe_pex_tee_centric_90_001:611979", "magi_pipe_pex_tee_centric_90_001:magi_pipe_pex_tee_centric_90_001:612015" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics

Types
  IFCPIPESEGMENTTYPE "Pipe Types:Feketeacél cső" | 12 occurrences | property sets: Identity Data, Other
  IFCVALVETYPE "AT3600-50" | 9 occurrences | property sets: Constraints, Dimensions, Graphics, Identity Data, Mechanical, Other
  IFCPIPESEGMENTTYPE "Pipe Types:PE - K1" | 38 occurrences | property sets: Identity Data, Other
  IFCVALVETYPE "321G-4010-50" | 3 occurrences | property sets: Constraints, Dimensions, Graphics, Identity Data, Mechanical, Other
  IFCPIPEFITTINGTYPE "Sanitary Sewerage Piping_Bend" | 9 occurrences | property sets: Constraints, Identity Data, Other
  IFCPIPEFITTINGTYPE "magi_pipe_fe_tee_centric_90_001" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Mechanical, Other
  IFCVALVETYPE "AT3600-50" | 9 occurrences | property sets: Constraints, Dimensions, Graphics, Identity Data, Mechanical, Other
  IFCVALVETYPE "321G-4010-50" | 3 occurrences | property sets: Constraints, Dimensions, Graphics, Identity Data, Mechanical, Other
  IFCPIPEFITTINGTYPE "Sanitary Sewerage Piping_Bend" | 3 occurrences | property sets: Constraints, Identity Data, Other
  IFCPIPEFITTINGTYPE "magi_pipe_pex_tee_centric_90_001" | 5 occurrences | property sets: Constraints, Dimensions, Identity Data, Mechanical, Other

Property sets
  Other | properties | on 76 objects (76 IFCFLOWSEGMENT)
    Category = "Pipes" (IFCLABEL)
    Family = "Pipe Types: PE - K1" (IFCLABEL)
    Family and Type = "Pipe Types: PE - K1" (IFCLABEL)
    Type = "Pipe Types: PE - K1" (IFCLABEL)
    Type Id = "Pipe Types: PE - K1" (IFCLABEL)
  Other | properties | on 24 objects (24 IFCFLOWSEGMENT)
    Category = "Pipes" (IFCLABEL)
    Family = "Pipe Types: Feketeacél cső" (IFCLABEL)
    Family and Type = "Pipe Types: Feketeacél cső" (IFCLABEL)
    Type = "Pipe Types: Feketeacél cső" (IFCLABEL)
    Type Id = "Pipe Types: Feketeacél cső" (IFCLABEL)
  Other | properties | on 18 objects (18 IFCFLOWCONTROLLER)
    Category = "Pipe Accessories" (IFCLABEL)
    Family = "AT3600-0001: AT3600-50" (IFCLABEL)
    Family and Type = "AT3600-0001: AT3600-50" (IFCLABEL)
    Type = "AT3600-0001: AT3600-50" (IFCLABEL)
    Type Id = "AT3600-0001: AT3600-50" (IFCLABEL)
  Other | properties | on 12 objects (12 IFCFLOWFITTING)
    Category = "Pipe Fittings" (IFCLABEL)
    Family = "pehd_bend_001: Sanitary Sewerage Piping_Bend" (IFCLABEL)
    Family and Type = "pehd_bend_001: Sanitary Sewerage Piping_Bend" (IFCLABEL)
    Type = "pehd_bend_001: Sanitary Sewerage Piping_Bend" (IFCLABEL)
    Type Id = "pehd_bend_001: Sanitary Sewerage Piping_Bend" (IFCLABEL)
  Other | properties | on 6 objects (6 IFCFLOWCONTROLLER)
    Category = "Pipe Accessories" (IFCLABEL)
    Family = "321G-0001: 321G-4010-50" (IFCLABEL)
    Family and Type = "321G-0001: 321G-4010-50" (IFCLABEL)
    Type = "321G-0001: 321G-4010-50" (IFCLABEL)
    Type Id = "321G-0001: 321G-4010-50" (IFCLABEL)
  Other | properties | on 5 objects (5 IFCFLOWFITTING)
    Category = "Pipe Fittings" (IFCLABEL)
    Family = "magi_pipe_pex_tee_centric_90_001: magi_pipe_pex_tee_centric_90_001" (IFCLABEL)
    Family and Type = "magi_pipe_pex_tee_centric_90_001: magi_pipe_pex_tee_centric_90_001" (IFCLABEL)
    Type = "magi_pipe_pex_tee_centric_90_001: magi_pipe_pex_tee_centric_90_001" (IFCLABEL)
    Type Id = "magi_pipe_pex_tee_centric_90_001: magi_pipe_pex_tee_centric_90_001" (IFCLABEL)
  Other | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCSYSTEM)
    Category = "Piping Systems" (IFCLABEL)
    Family = "Piping System: D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK" (IFCLABEL)
    Family and Type = "Piping System: D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK" (IFCLABEL)
    Type = "Piping System: D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK" (IFCLABEL)
    Type Id = "Piping System: D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK" (IFCLABEL)
  Other: 8 more contents on 3 objects not shown
  Mechanical | properties | on 12 objects (12 IFCFLOWCONTROLLER)
    Loss Method = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Hydronic Return" (IFCTEXT)
    System Name = "D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK 3" (IFCTEXT)
    System Type = "Piping System: D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK" (IFCLABEL)
    isMeasuringValve = FALSE (IFCBOOLEAN)
  Mechanical | properties | on 12 objects (12 IFCFLOWCONTROLLER)
    Loss Method = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Hydronic Return" (IFCTEXT)
    System Name = "D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK 2" (IFCTEXT)
    System Type = "Piping System: D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK" (IFCLABEL)
    isMeasuringValve = FALSE (IFCBOOLEAN)
  Mechanical | properties | on 6 objects (6 IFCFLOWFITTING)
    Loss Method = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Hydronic Return" (IFCTEXT)
    System Name = "D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK 3" (IFCTEXT)
    System Type = "Piping System: D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK" (IFCLABEL)
  Mechanical | properties | on 6 objects (6 IFCFLOWFITTING)
    Loss Method = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Hydronic Return" (IFCTEXT)
    System Name = "D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK 2" (IFCTEXT)
    System Type = "Piping System: D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK" (IFCLABEL)
  Mechanical | properties | on 3 objects (3 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Method = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
    MC_R1 = 37.5 (IFCLENGTHMEASURE) [MILLI METRE]
    MC_R3 = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Hydronic Return" (IFCTEXT)
    System Name = "D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK 3" (IFCTEXT)
    System Type = "Piping System: D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK" (IFCLABEL)
  Mechanical | properties | on 3 objects (3 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Loss Method = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
    MC_R1 = 37.5 (IFCLENGTHMEASURE) [MILLI METRE]
    MC_R3 = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Hydronic Return" (IFCTEXT)
    System Name = "D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK 2" (IFCTEXT)
    System Type = "Piping System: D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 0.0153152645092148 (IFCAREAMEASURE) [SQUARE_METRE]
    Connection Type = "Generic" (IFCTEXT)
    Diameter = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Invert Elevation = 4174.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "Feketeacél cső" (IFCLABEL)
    Pipe Segment = "Feketeacél cső" (IFCLABEL)
    Roughness = 0.0450000017881393 (IFCLENGTHMEASURE) [MILLI METRE]
    Schedule/Type = "Pipe Schedule Types: Schedule 40" (IFCLABEL)
    Section = 1 (IFCINTEGER)
    Segment Description = "Feketeacél" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Hydronic Return" (IFCTEXT)
    System Name = "D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK 3" (IFCTEXT)
    System Type = "Piping System: D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK" (IFCLABEL)
  Mechanical | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Area = 0.0223764803480255 (IFCAREAMEASURE) [SQUARE_METRE]
    Connection Type = "Generic" (IFCTEXT)
    Diameter = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Invert Elevation = 4174.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "Feketeacél cső" (IFCLABEL)
    Pipe Segment = "Feketeacél cső" (IFCLABEL)
    Roughness = 0.0450000017881393 (IFCLENGTHMEASURE) [MILLI METRE]
    Schedule/Type = "Pipe Schedule Types: Schedule 40" (IFCLABEL)
    Section = 1 (IFCINTEGER)
    Segment Description = "Feketeacél" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Hydronic Return" (IFCTEXT)
    System Name = "D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK 3" (IFCTEXT)
    System Type = "Piping System: D3040.20.002-FŰTÉSI/HŰTÉSI VISSZATÉRŐ VEZETÉK" (IFCLABEL)
  Mechanical: 52 more contents on 98 objects not shown
  Identity Data | properties | on 64 objects (64 IFCFLOWSEGMENT)
    Comments = "Padlófűtés" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "2" (IFCTEXT)
    Productdata = "© Progman Oy, all rights reserved" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "5" (IFCTEXT)
    Productdata = "© Progman Oy, all rights reserved" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "7" (IFCTEXT)
    Productdata = "© Progman Oy, all rights reserved" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "9" (IFCTEXT)
    Productdata = "© Progman Oy, all rights reserved" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "24" (IFCTEXT)
    Productdata = "© Progman Oy, all rights reserved" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "26" (IFCTEXT)
    Productdata = "© Progman Oy, all rights reserved" (IFCTEXT)
  Identity Data: 28 more contents on 21 objects not shown
  Constraints | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Bottom Elevation = 171.5 (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 01 Level" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 228.50000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Bottom Elevation = 171.500000000003 (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 01 Level" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 228.50000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Bottom Elevation = 250.000000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 250.000000000003 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 544.999999374546 (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 01 Level" (IFCLABEL)
    Start Middle Elevation = 544.999999374546 (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 544.999999374547 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Bottom Elevation = 654.999997944029 (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 654.999997944032 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 725.000000000006 (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 01 Level" (IFCLABEL)
    Start Middle Elevation = 725.000000000006 (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 725.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Bottom Elevation = 1054.99999794403 (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 1054.99999794403 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 1950.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 01 Level" (IFCLABEL)
    Start Middle Elevation = 1950.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 1950.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Bottom Elevation = 875.000000000007 (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 875.000000000007 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 944.999999374547 (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 01 Level" (IFCLABEL)
    Start Middle Elevation = 944.999999374547 (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 944.999999374547 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Bottom Elevation = 10050. (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 13750. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 10050. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 01 Level" (IFCLABEL)
    Start Middle Elevation = 10050. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 13750. (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Bottom Elevation = 171.5 (IFCLENGTHMEASURE) [MILLI METRE]
    End Middle Elevation = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Justification = "Center" (IFCIDENTIFIER)
    Middle Elevation = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: 02 Level" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Middle Elevation = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Elevation = 228.50000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Justification = "Middle" (IFCIDENTIFIER)
  Constraints: 47 more contents on 113 objects not shown
  Dimensions | properties | on 18 objects (18 IFCFLOWCONTROLLER)
    Area = 0.0257497783989643 (IFCAREAMEASURE) [SQUARE_METRE]
    Maximum Size = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Size = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "50 mmø-50 mmø" (IFCTEXT)
    Use Minimum Symbol Size = TRUE (IFCBOOLEAN)
    Volume = 7.74971215746629E-6 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    ang2D = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Dimensions | properties | on 12 objects (12 IFCFLOWSEGMENT)
    Inside Diameter = 51.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 97.5000020560566 (IFCLENGTHMEASURE) [MILLI METRE]
    Outside Diameter = 57. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "50 mmø" (IFCTEXT)
  Dimensions | properties | on 12 objects (12 IFCFLOWSEGMENT)
    Inside Diameter = 51.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 142.453098255477 (IFCLENGTHMEASURE) [MILLI METRE]
    Outside Diameter = 57. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "50 mmø" (IFCTEXT)
  Dimensions | properties | on 12 objects (12 IFCFLOWSEGMENT)
    Inside Diameter = 44. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 294.999999374543 (IFCLENGTHMEASURE) [MILLI METRE]
    Outside Diameter = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "50 mmø" (IFCTEXT)
  Dimensions | properties | on 12 objects (12 IFCFLOWSEGMENT)
    Inside Diameter = 44. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 70.0000020559741 (IFCLENGTHMEASURE) [MILLI METRE]
    Outside Diameter = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "50 mmø" (IFCTEXT)
  Dimensions | properties | on 12 objects (12 IFCFLOWSEGMENT)
    Inside Diameter = 44. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 69.9999993745401 (IFCLENGTHMEASURE) [MILLI METRE]
    Outside Diameter = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "50 mmø" (IFCTEXT)
  Dimensions | properties | on 12 objects (12 IFCFLOWFITTING)
    Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    L1 / tan(Angle / 2) = 50.0000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    L1 = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Size = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Size = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    ND = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    NR = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "50 mmø-50 mmø" (IFCTEXT)
    Volume = 0.000154207934891838 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 6 objects (6 IFCFLOWCONTROLLER)
    Area = 0.0127037191363035 (IFCAREAMEASURE) [SQUARE_METRE]
    Maximum Size = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Size = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "50 mmø-50 mmø" (IFCTEXT)
    Use Minimum Symbol Size = TRUE (IFCBOOLEAN)
    Volume = 5.14898377404695E-6 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    ang2D = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Dimensions: 19 more contents on 49 objects not shown
  Insulation | properties | on 84 objects (84 IFCFLOWSEGMENT)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "50 mmø" (IFCTEXT)
  Insulation | properties | on 36 objects (24 IFCFLOWCONTROLLER, 12 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "50 mmø-50 mmø" (IFCTEXT)
  Insulation | properties | on 16 objects (16 IFCFLOWSEGMENT)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "75 mmø" (IFCTEXT)
  Insulation | properties | on 6 objects (6 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "75 mmø-75 mmø-50 mmø" (IFCTEXT)
  Mechanical - Flow | properties | on 74 objects (74 IFCFLOWSEGMENT)
    Additional Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow State = "Laminar" (IFCIDENTIFIER)
    Friction = 0. (IFCREAL)
    Friction Factor = 0. (IFCREAL)
    Pressure Drop = 0. (IFCPRESSUREMEASURE) [PASCAL]
    Relative Roughness = 0. (IFCREAL)
    Reynolds Number = 0. (IFCREAL)
    Velocity = 0. (IFCLINEARVELOCITYMEASURE) [derived]
  Mechanical - Flow | properties | on 26 objects (26 IFCFLOWSEGMENT)
    Additional Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow State = "Laminar" (IFCIDENTIFIER)
    Friction = 0. (IFCREAL)
    Friction Factor = 0. (IFCREAL)
    Pressure Drop = 0. (IFCPRESSUREMEASURE) [PASCAL]
    Relative Roughness = 0.000878906284924597 (IFCREAL)
    Reynolds Number = 0. (IFCREAL)
    Velocity = 0. (IFCLINEARVELOCITYMEASURE) [derived]
  Phasing | properties | on 142 objects (100 IFCFLOWSEGMENT, 24 IFCFLOWCONTROLLER, 18 IFCFLOWFITTING)
    Phase Created = "Phase 1" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 38 objects (38 IFCFLOWSEGMENT)
    Reference = "PE - K1" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 18 objects (18 IFCFLOWCONTROLLER)
    Reference = "AT3600-50" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 12 objects (12 IFCFLOWSEGMENT)
    Reference = "Feketeacél cső" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 12 objects (12 IFCFLOWFITTING)
    Reference = "Sanitary Sewerage Piping_Bend" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 6 objects (6 IFCFLOWCONTROLLER)
    Reference = "321G-4010-50" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 5 objects (5 IFCFLOWFITTING)
    Reference = "magi_pipe_pex_tee_centric_90_001" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWFITTING)
    Reference = "magi_pipe_fe_tee_centric_90_001" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 12 objects (12 IFCFLOWSEGMENT)
    Roughness = 0.0450000017881393 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 6 objects (6 IFCFLOWSEGMENT)
    Length = 97.5000020560566 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 6 objects (6 IFCFLOWSEGMENT)
    Length = 142.453098255477 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 6 objects (6 IFCFLOWSEGMENT)
    Length = 294.999999374543 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 6 objects (6 IFCFLOWSEGMENT)
    Length = 70.0000020559741 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 6 objects (6 IFCFLOWSEGMENT)
    Length = 69.9999993745401 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 3 objects (3 IFCFLOWSEGMENT)
    Length = 53.7500000000051 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 3 objects (3 IFCFLOWSEGMENT)
    Length = 3900. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 3700. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment: 9 more contents on 12 objects not shown
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    InvertElevation = 4174.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 97.5000020560566 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    InvertElevation = 4174.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 142.453098255477 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    InvertElevation = 4250. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 294.999999374543 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    InvertElevation = 4654.99999794403 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 70.0000020559741 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    InvertElevation = 4875.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 69.9999993745401 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    InvertElevation = 14050. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 3700. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    InvertElevation = 8174.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 97.5000020560566 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    InvertElevation = 8174.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 142.453098255477 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment: 23 more contents on 34 objects not shown
  Pset_ProductRequirements | properties | on 50 objects (50 IFCFLOWSEGMENT)
    Category = "Pipes" (IFCLABEL)
  Pset_ProductRequirements | properties | on 24 objects (24 IFCFLOWCONTROLLER)
    Category = "Pipe Accessories" (IFCLABEL)
  Pset_ProductRequirements | properties | on 18 objects (18 IFCFLOWFITTING)
    Category = "Pipe Fittings" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "01 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "02 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "03 Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 38 objects (38 IFCFLOWSEGMENT)
    Reference = "PE - K1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 18 objects (18 IFCFLOWCONTROLLER)
    Reference = "AT3600-50" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 12 objects (12 IFCFLOWSEGMENT)
    Reference = "Feketeacél cső" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 12 objects (12 IFCFLOWFITTING)
    Reference = "Sanitary Sewerage Piping_Bend" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 6 objects (6 IFCFLOWCONTROLLER)
    Reference = "321G-4010-50" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCFLOWFITTING)
    Reference = "magi_pipe_pex_tee_centric_90_001" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFLOWFITTING)
    Reference = "magi_pipe_fe_tee_centric_90_001" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 18 objects (18 IFCFLOWCONTROLLER)
    Manufacturer = "Armatec" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 6 objects (6 IFCFLOWCONTROLLER)
    Manufacturer = "Axel Larsson" (IFCLABEL)
  Graphics | properties | on 42 objects (24 IFCFLOWCONTROLLER, 18 IFCFLOWFITTING)
    Use Annotation Scale = FALSE (IFCBOOLEAN)
  Graphics | properties | on 2 type objects
    magiFamilyGeom = "MagiCAD_AT3600-50" (IFCLABEL)
  Graphics | properties | on 2 type objects
    magiFamilyGeom = "MagiCAD_321G-4010-50" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "01 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "02 Level" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "03 Level" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 3 (IFCINTEGER)
  Constraints(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Other(Type) | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)

Other addresses and roles
  2 x postal address: "Enter address here", "Boston", "MA"